E U R O P E AN S O U T H E R N O B S E R VAT ORY

Organisation EuropØenne pour des Recherches Astronomiques dans l’HØmisphŁre Austral Europ�ische Organisation f�r astronomische Forschung in der s�dlichen Hemisph�re

VLT PROGRAMME

VERY LARGE TELESCOP E

LCU Common Software --- LCU Server Framework

User Manual

Doc. No.: VLT-MAN-ESO-17210-2252 Issue: 1.0 Date: 2000-10-25

Prepared: P.Duhoux 2000-10-25

Name Date Signature

Approved: B. Gustafsson

Name Date Signature

Released: G. Raffi

Name Date Signature

VLT PROGRAMME * TELEPHONE: (089) 3 20 06-0 * FAX: (089) 3 20 06 514

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

2 of 81

CHANGE RECORD

ISSUE DATE SECTION/PAGE

AFFECTED REASON/INITIATION

DOCUMENTS/REMARKS

1.0 2000-10-25 All First preparation

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 3 of 81

TABLE OF CONTENTS

1 INTRODUCTION 5 1.1 Purpose & Scope 5 1.2 Applicable Documents 5 1.3 Reference Documents 6 1.4 Acronyms 7 1.5 Stylistic Conventions 7 1.5.1 Text 7 1.5.2 Diagrams 7

2 USER MANUAL 8 2.1 Introduction 8 2.2 LCU Server Framework 8 2.2.1 lsf: the LCU Server Framework 8 2.2.2 lsftpl : the LCU Server Application Template 13 2.3 LCU Server Application 15 2.3.1 Module Creation 15 2.3.2 Module Configuration 15 2.3.3 Specific Implementation 18 2.3.4 Scan Links 19 2.3.5 Database Configuration 19 2.3.6 Default panel & UIF widget 20 2.3.7 Application Makefiles 20 2.3.8 Implementation Rules for the Command Handlers 21 2.3.9 Hook functions 21 2.3.10 Miscellaneous 24

3 REFERENCE 25 3.1 Utilities 25 3.1.1 lsf(1) 25 3.1.2 lsfCreate(1) 30 3.1.3 lsfConfig(1) 31 3.1.4 lsfBackup(1) 33 3.2 Code 34 3.2.1 lsfServer(3) 34 3.2.2 lsfStandard(3) 39 3.2.3 lsfSignalHandlers(3) 41 3.2.4 lsfControl(3) 42 3.2.5 lsfDevice(3) 45 3.2.6 lsfSignal(3) 47 3.2.7 lsfMotor(3) 50 3.2.8 lsfSerial(3) 53 3.2.9 lsfTaskDev(3) 56 3.2.10 lsfSoftDev(3) 59 3.3 Database Classes 62 3.3.1 lsfTemplate.db 62 3.3.2 lsfDB_SERVER(5) 64 3.3.3 lsfDB_CONTROL(5) 65 3.3.4 lsfDB_DATA(5) 66 3.3.5 lsfDB_DEVICE(5) 67 3.3.6 lsfDB_SIGNAL(5) 68 3.3.7 lsfDB_MOTOR(5) 70

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

4 of 81

3.3.8 lsfDB_SERIAL(5) 71

3.3.9 lsfDB_TASKDEV(5) 72

3.3.10 lsfDB_SOFTDEV(5) 73

3.4 Include Files 74

3.4.1 lsfDefines.h 74

4 INSTALLATION GUIDE 77

4.1.1 WS Environment 77

4.1.2 LCU Environment 77

4.1.3 Scan Links 79

4.1.4 Verification 80

4.1.5 Database configuration 80

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 5 of 81

1 Introduction

1.1 P urpose & Scope

This document describes the usage of the LCU Server Framework lsf from a programmatic point of view. It is intended to provide all the necessary information for an application developer to create, configure, customize and install LCU Server applications. It describes all the necessary steps that must be performed for the implementation of a new Software Device. The intended readers are application developers of VLT Software who need to develop, test or maintain LCU Server Applications, based on this framework.

The author assumes the reader has a good knowledge of the VLT Standards and Software Engineering practices, especially experience with Real-Time and Object Oriented concepts and UML Notation would be an asset.

Beside the Introduction, the document is built in 3 parts:

• the User Manual describes the concepts and usage of the LCU Server Framework • the Reference section provides the necessary man-pages for all the available scripts, commands and code • the Installation Guide explains how to install a new LCU Server Application in the VLT environments

Last modified: Thu Oct 26 12:50:45 METDST 2000

1.2 Applicable Documents

The following documents, of the exact issue shown, form part of this document to the extend specified herein. In the event of conflict between the documents referenced herein and the content of this issue, the content of this document shall be considered as a superseding requirement.

Reference Document Number Issue Date Title

[AD 01] VLT-SPE-ESO-10000-0011 2.0 30/09/1992 VLT Software Requirements Specifications [AD 02] VLT-PRO-ESO-10000-0228 1.0 10/03/1993 VLT Software Programming Standards [AD 05] VLT-MAN-ESO-17200-0888 1.0 17/08/1995 VLT Common Software Overview [AD 06] VLT-MAN-ESO-17210-0642 1.11 22/11/1999 VLT Common Software Installation Manual

[AD 07] VLT-MAN-ESO-17210-0855 3.0 30/10/1998

VLT Software Environments Common Configuration User Manual

[AD 08] VLT-MAN-ESO-17210-0667 1.0 03/12/1996

Guidelines for the Development of VLT Application Software

[AD 09] VLT-SPE-ESO-17210-2051 1.0 2000-03-10

LCU Common Software - LCU Server Framework Detailed Design

ESO_{LCU Common Software}

LCU Server Framework

User Manual

Doc.

Issue

Date

Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25

6 of 81

1.3 Reference Documents

The reference documents contain background information required to fully understand the structure of this document, the terminology used, the software environment in which the product shall be integrated and the interface characteristics to the external systems.

VLT Project Software documents are available from the ESO VLT Project Archive or online at the following URL:

http://www.eso.org/projects/vlt/sw-dev/ftp/index.html

Reference Document Number Issue Date Title

[RDV 01] VLT-MAN-ESO-17210-0619 1.6 20/10/1999 VLT Central Control Software - User Manual

[RDV 02] VLT-MAN-SBI-17210-0001 3.5 20/10/1999 LCU Common Software - User Manual

[RDV 03] VLT-MAN-ESO-17210-0707 1.4 20/10/1999 CCS On-Line Database Loader - User Manual

[RDV 04] VLT-SPE-ESO-17230-0819 1.3 18/09/1997 Mode Switching - Design Description

[RDV 05] VLT-MAN-ESO-17210-0600 1.7 02/10/1998 LCC Motor Control Module - User Manual

The following non-VLT documents are referenced in the document:

Reference Title Authors P ublisher, Date

[RD 01] IEEE Std 1012, Standard for Software

Verification and Validation Plans 1986

[RD 02] IEEE Std 830, Recommended Practice for

Software Requirements Specifications 1993

[RD 03] IEE (UK), Guidelines for the Documentation of

Software in Industrial Computer Systems 1985

[RD 04] The Unified Modeling Language Reference

Manual J. Rumbaugh, G. Booch,

I. Jacobson Addison-Wesley,

1998

[RD 05] The Unified Modeling Language User Guide G. Booch, J. Rumbaugh,

I. Jacobson Addison-Wesley,

1998

[RD 06] The Unified Software Development Process I. Jacobson, G. Booch,

J. Rumbaugh Addison-Wesley,

1999

[RD 07] Real-Time UML - Developing Efficient Objects

For Embedded Systems B. Douglas Addison-Wesley,

1998

[RD 08] Design Patterns - Elements of Reusable Object-

Oriented Software E. Gamma, R. Helm,

R. Johnson and J. Vlissides Addison-Wesley,

1994

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 7 of 81

1.4 Acronyms

This document employs several abbreviations and acronyms to refer concisely to an item, after it has been introduced. The following list is aimed to help the reader in recalling the extended meaning of each short expression:

[AD xx] Applicable Document #xx
CCS Central Common Software
DB Database
ESO European Southern Observatory
I/O Input/Output
LAN Local Area Network
LCC LCU Common Software
LCU Local Control Unit
MCM Motor Control Module (part of LCC)
OLDB On-line Database
OO Object Oriented
[RD xx] Reference Document #xx
RT Real-Time
TIM Time Interface Module
UC Use Case
UML Unified Modeling Language
VME Versa Module Eurocard
WS (Unix) Work Station

1.5 Stylistic Conventions

1.5.1 Text

The following styles are used:

• bold : in the text, for commands, filenames, pre- and suffixes as they have to be typed. • italic : in the text, for parts that have to be substituted with the real content before typing. • teletype : for examples. • <name> : in the examples, for parts that have to be substituted with the real content before typing.

1.5.2 Diagrams

All diagrams are based on the UML notation, as described in [RD 04] and given in Appendix. Besides the classical class notation, three dedicated icons are used throughout the class diagrams for representing the UML standard class stereotypes ([RD 06] pp. 183ff) and shown below:

• <<boundary>>: model interactions between the system and its actors. • <<entity>>: model information and associated behavior of phenomenon, concept such as a real-life objects; often persistent.

• <<control>>: represent coordination, sequencing, transactions and control of other objects; often used to encapsulate the control related to a use-case.

Last modified: Thu Oct 26 14:15:25 METDST 2000

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

8 of 81

2 User Manu al

2.1 Introduction

In this chapter, the concept of the LCU Server Framework will be described. This section is followed by the practical description of its usage through the whole creation and customization process of a new LCU

Server Application.

Naming Conventions: In this chapter, the following naming conventions apply: the generic names devtype and Devtype differ only by the case of the first letter (lower/upper). The first case indicates the name of the device type, the latter is the name of the device type when concatenated with the module prefix as in appDevtype.

2.2 LCU Server Framework

The intent, motivation and consequences of the framework have been discussed in detail in [AD 09]. The framework implements the minimum behavior for all the Standard Commands and offers the expected extensibility, flexibility and changeability while defining a fixed architecture and improving the overall maintainability as most of the code is provided and reused.

2.2.1 lsf: the LCU Server Framework

The framework consists in a collection of reusable components that implement the standard behaviour for a number of devices. It provides a unique and fully re-entrant set of common procedures that need not be duplicated by new applications.

As of this issue, lsf supports the following devices:

• I/O signals: digital and analog signals based resp. on the VLT standard Acromag AVME 948x

Digital I/O and VMIVME-3111 Analog I/O VME boards

• motors: any kind of motor as supported by MCM

• serial communication links: based on the VxWorks tyCo driver and on the VLT standard esd

ISER8 Serial Interface Board.

• tasks: any periodic task running in background as part of the Software Device

• software devices: any lsf-based sub-Software Device running on the same LCU.

Architecture: The purpose of a framework is to impose the architecture of the applications based on and to provide the implementation of the standard behaviour. The application is consequently responsible for implementing the specialized functionality as of its design.

The architecture is hierarchical: The server object lsfServer is responsible for handling the application global data and hosts the commands of the application; these commands might involve no device (pure software command) or devices of various types (combined command). The actual control of the devices is performed from within the object lsfControl that dispatches the standard commands to the respective devices. Finally for each device type, an object lsfDeviceType implements the commands of this type of device.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 9 of 81

Comma nd Interpreter

lsf Init All

<<a ctive>>

LCU Server 1

lsfCONTROL_ENTRY

na me : vltBYTES20 type : In teger sta rtPhase : Integer stopP ha se : Integer simula tion : Boolea n ignored : Boolean lsf SERVER_DATA sta te su bState initia lized simula tion timeout serverNam e

<<control>>

1 +serverDa ta

lsf Monitor

lsfMon itor() lsfWa keu pMonitor()

<<active>> 1

lsf CONTROL_DATA nu mDevices : Integer[]

<<control>>

1..n

+deviceTa ble

1 +controlDa ta 1

Comma nd Handler

23..n

lsfDEVICE_ENTRY

sta te : Integer = 1 subSta te : Integer = 0 init : Boolea n = F simu la tion : Boolean = F timeou t : In teger = 120 s

devna meCon structor()

(from Devices)

Device

<<Device>>

0..n0..n

qu ery

1..n

+deviceDa ta lsfDEVICE_DATA

numDevices : Integer deviceNa m es[] : String

ESO_{LCU Common Software}

LCU Server Framework

User Manual

Doc.

Issue

Date

Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25

10 of 81

Standard Behaviour: The standard commands are implemented within the framework. They define the standard behaviour of each standard command for each type of device. The standard behaviour is edicted in [RDV 02] for Software Devices and State management. The standard behaviour can not be modified but only extended by means of dedicated hooks functions, which are application specific and implement additional actions required by the application design (e.g. set a particular I/O signal prior to go Online).

States and Sub-States: Each device is characterized by its state and sub-state. The state is defined by

LCC ([RDV 02]) and takes the values OFF, LOADED, STANDBY or ONLINE.

Each group of devices of a type is as well characterized by a state and sub-state value; the state is set as being the lowest state of all the devices of this group.

The global application state is then the lowest state value of all the devices.

Cold Start

OF F

Im plicit transition when switching to any lower sta te.

LOADED

Idle - Not

Initialized

Initializing

Idle-

Initialized

Error

ONLINE

Idle

Active

Error STANDBY

All equipem ent is powered-off or in low-power m ode, but those required for sa fety or thermal stability and preventing any degradation of the system .

ONLINE

STANDBY

STANDBY / STOP

[ any error ]

[ LCU boot OK ]

/ log error

INIT | STANDBY | ONLINE

STOP

[ som e step failed ]

[ all init step OK ]

[ any error ]

/ log error ONLINE

Specific Comm and

STOP | Com pletion OK

[ action failure ]

Transcient sub-state:

- the error is logged

- the sub-state resets to Idle

STANDBY ONLINE

All equipem ent is powered-off or in low-power m ode, brakes cla mped.

EXIT | KILL / OFF

SIMULAT | STOP SIM | TEST / STOP

INIT / STOP

OF F / STOP

SELFTST

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 11 of 81

The sub-state is used to indicate the detailed activity of a device, or group of devices; the following substates have been introduced:

• Idle: the device is inactive • Error: an error has occured • Timeout: the requested action has timed out • Initializing: the device is performing the initialization procedure • Monitoring: monitoring is active in background • Moving: for motors only when performing a motion • Active: any other activity like e.g. Waiting for an event, in a Control Loop etc...

The 2 sub-states Error and Timeout are transcient states that reset to Idle on recovery, or on next request. The global sub-state of the software device is set to:

• Idle: when all the devices are inactive • Error: if one device went in error. • Timeout: if one device timed out. • Initializing: if one device is initializing • Active: if one device or more is active

Database: All relevant configuration and runtime data is stored in the OLDB of the LCU, which is partly mirrored on the WS so as to enable the use of the scan system. Each type of device is mapped in the database by a dedicated class. All the device classes are derived from the base abstract class lsfDB_DEVICE as depicted in the class hierarchy:

lsfDB_AN ALOG channel : Integer gain : ioGAIN conversionFactor : Float lowerRange : Float higherRange : Float simValue : Float dataBits : Integer = 8 stopBits : Integer = 1 parity : Integer = 1 handShake : Integer = 1 rxMode : Integer = 0 bufferLength : Integer = 512 lsfDB_MOTOR motor : motMOTOR lsfDB_SIGN AL deviceN ame : lccDEVICE_N AME direction : ioIN _OU T lsfDB_TASKDEV star tState : Integer = lsfSTATE_ON LIN E ignoreStop : Boolean = TRU E timerN um : Integer = -1 period : Integer = 1000 ms priority : Integer = 80 stackSize : Integer = 30 kB lsfDB_EN CODER deviceN ame : lccDEVICE_N AME

lsfDB_N ETWORK deviceN ame : lccDEVICE_N AME ipN ame : String ipAddr : Integer gateway : Integer lsfDB_DATA lsfDB_CON TROL_EN TRY name : String type : String star tPhase : Integer = 0 stopPhase : Integer = 0 simulation : Boolean = F ignored : Boolean = F lsfDB_SERVER

subState : Integer = 0 simulation : Boolean = 0 initialized : Boolean = 0 timeout : Integer = 120 s lsfDB_CON TROL 1..n

+deviceTable

0..10..1

1..n

+<deviceType>

Note that a Software Device is a sub-class of lsfDB_SOFTDEV, thus allowing recursive construction: a Software Device can be a sub-Software Device of another one.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

12 of 81

The structure of the database is fixed as illustrated in the diagram below:

lsfDB_SERVER lsfDB_DEVICE lsfDB_MOTOR lsfDB_SERIAL lsfDB_SIGNAL lsfDB_SOFTDEV lsfDB_TASKDEV lsfDB_NETWORK lsfDB_ENCODER

lsfDB_CONTROL

:mot_1..n :com_1..n :ios_1..n :swd_1..n :tsk1..n :enc1..n :net1..n

:motor

1..n1..n

:serial

1..n1..n

:signal

1..n1..n

:softdev

1..n1..n

:taskdev

1..n1..n

:encoder

1..n1..n

:network

1..n1..n

:control

0..10..1 0..10..1 0..10..1 0..10..1 0..10..1 0..10..1 0..10..1

:data

lsfDB_ROOT

<<alias>> LSF

0..10..1 1 lsfDB_DATA

Note the multiplicity of the various instances as a means to scale the database to the exact needs of the application.

Application Data: The class lsfDB_DATA is an abstract class. It does not contain any attribute as it is intended to be specialized (by sub-classing) to the needs of the application. This class has been introduced so as to allow the application to store data that shows following characteristics at a known location:

• the data is not strictly device dependent (e.g. temperatures, or telemetry values), or shall be hardware independent (i.e. should a thermometer device be exchanged from a device with digital interface to a one with serial interface)

• the data might be accessed from within another device (e.g. a background task) for further processing

• the data might need to be scanned to the WS independently on the devices producing it.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 13 of 81

2.2.2 lsftpl : the LCU Server Application Template

The module lsftpl is a template application based on lsf that provides an implementation template for all available device types. In particular, it gives examples of ACI and API functions for signals and motors for addressing one or all devices of this type. The template implements the control of 16 devices: 8 I/O signals (4 analogue and 4 digital where from 2 input and 2 output signals), 2 motors, 3 serial communication links (2 using the ISER 8 board, and one

/tyCo device), 2 sub-ordinated software devices (swdtst1 and swdtst2) and 1 task device performing

periodic monitoring) as illustrated in the class diagram below:

TRS

LCU Server

<<fram ework>>

(from Sta ndard Package)

User

M1 M2 com1 com2

tyCo1

DI2 DI3

DO1 DO4

AI1 AI8

AO3 AO4 swd1tst swd2tst APP <<SubSystem>>

appMotor

(from appMotor)

<<Device>> appSerial

(from appSerial)

<<Device>> appSignal

(from appSignal)

<<Device>> appSoftDev

(from appSoftdev)

<<Device>>

appBgTask

(from appTaskdev)

<<active>> appServer 1

1_1 1

1 appTaskDev

(from appTaskdev)

<<Device>>

1

1

LCU Server Template

<<tem plate>>

(from Sta ndard Package)

ESO_{LCU Common Software}

LCU Server Framework

User Manual

Doc.

Issue

Date

Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25

14 of 81

It implements the functionality as shown in the Use Case diagram:

M2 com2

AI1

DO4

AO4

DI3

AI8

AO3

DI2

DO1 tyCo1 com1 an Encoder

M1 a Network Port swd1tst

Read Analog Signal

Write Analog Signal

Read Digital Signal

Write Digital Signal

Read Serial Comm unication Port

Write Serial Com munication Port

Read Encoder Head

Execute Main Command

Move Motor Absolute

Read Netw ork Communication Port

Write N etwork Com munication Port

Forward Comm and

SOFTCMD <<message>>

User

RASIG <<m essage>>

WASIG <<m essage>>

RDSIG <<m essage>>

WDSIG <<m essage>>

RSCOM <<m essage>>

WSCOM <<m essage>>

RHEAD <<message>>

MAIN CMD <<message>>

MOVEA <<message>>

RECOM <<m essage>>

WECOM <<m essage>>

SOFTCMD

<<m essage>> swd2tst

SOFTCMD <<m essage>>

Execute Com mand

SWDCMD

<<m essage>> swd2tstSwdCommand

<<call>>

N.B.: as of this version, both the encoder and network devices are not yet supported.

The following section describes all the steps necessary to create a new application from this template.

ESO

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

17 of 81

The effective configuration of the LCU Server Application app is made by means of the utility lsfConfig(1).

It performs following steps:

1. Parse the configuration file app/ws/config/app.cfg and display all the devices by type and the commands by group

2. Generate the include file app/lcu/include/appDeviceList.h containing the macro definition of all devices

3. Generate the database file app/lcu/dbl/app.db for the instantiation of the database point.

4. Generate the makefile app/lcu/src/Makefile

5. Generate the CDT partial files app/lcu/src/appPublic.cdt, app/lcu/src/appMaintenance.cdt and app/lcu/src/appTest.cdt. The files are created only if at least one command has been declared in this group.

6. Generate the CIT partial files app/lcu/src/app<Devtype>.cit for each referenced device type

Devtype.

7. Move all the unused files to app/lcu/tmp

(The unused files are the files associated to the control of the device types not referenced in the configuration file. They are moved to this directory prior to be removed by the user when preparing for archive.)

8. Generate the log file app/ChangeLog and add an entry for the configuration sequence.

Important Note: The utility lsfConfig shall be called once as its actions are destructive for some files.

Any application dependent modification made to the partial CDT files will be lost during this process, as these files are re-created. A posteriori addition of a device of a new type is not supported.

Example:

> lsfConfig app

Parse file ’app/ws/config/app.cfg’ ... done

Found 1 device:

     1 Motor    : NDF

Found 1 PUBLIC command:

     1 Motor    : SETNDF

Found 0 MAINTENANCE command

Found 0 TEST command

Generate ’app/ws/config/app.dbcfg’ ... done

Generate ’app/lcu/include/appDeviceList.h’ ... done

Generate ’app/lcu/dbl/app.db’ ... done

Generate ’app/lcu/src/Makefile’ ... done

Generate ’app/lcu/src/appPublic.cdt’ ... done

Generate ’app/lcu/src/appMotor.cit’ ... done

Move unused files to ./lcu/tmp ... done

Add change log entry ... done

>>> Remember to edit the CDT files ...

Module configuration for ’app’ ... done"

>

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 18 of 81

2.3.3 Specific Implementation

After the module has been tailored to the needs of the application, some files need be edited to implement the behaviour and specify the interfaces as of the design.

• app/lcu/src/appPublic.cdt,

app/lcu/src/appMaintenance.cdt,
app/lcu/src/appTest.cdt: For each command the parameters and replies must be described.

• app/lcu/dbl/appDB_DEVICE.class: Each application specific device class must be defined as a sub-class of the corresponding device type lsfDB_DEVTYPE • app/lcu/dbl/appDB_DATA.class: If any extra data storage is needed in the database by the application, the class appDB_DATA must be described in this file • app/lcu/include/app<Devtype>.h: for each referenced device type, the prototypes of the API functions associated to the commands must be declared. The file

app/lcu/include/appServer.h is also subject to modification.

The API function shall be named following the convention for the ACI function names without the leading I.

• app/lcu/src/app<Devtype>.c: Each API function must be implemented in the respective file. • app/lcu/src/app<Devtype>Interface.c: Each ACI function must be implemented in the respective file.

For the sake of clarity, one might group the API functions dedicated to one specific device into one separate file. These files may be included into the device type associated file.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

19 of 81

The class diagram shown below depicts the device control structure for a specific command:

lsfDEVICE_DATA

<<ACI>>IappDeviceSpecificCommand()

app Command Interpreter

2.3.7 Application Makefiles

The WS part is built as described in app/ws/src/Makefile. It makes the panel app/ws/src/appgui.pan and installs the two configuration files app/ws/config/app.scan and
app/ws/config/app.dbcfg under $XXXROOT/config.

Example:

> cd app/ws/src

> make all install

 ...

 . . . ’all’ done

 ...

 . . . installation done

>

The LCU part is built as described in app/lcu/src/Makefile.

It invokes 3 utilities prior to building the code (target "all"):

• lsfMakeCIT: merge all the partial CIT files app/lcu/src/app*.cit and the common CIT file

$XXXROOT/vw/CIT/lsfCommon.cit into app/lcu/CIT/appServer.cit;

• lsfMakeCDT: merge all the partial CDT files app/lcu/src/app*.cdt and the common CDT files

$XXXROOT/CDT/lsf*.cdt into app/lcu/CDT/appServer.cdt;

• lsfMakeINC: generate all the files app/lcu/include/app*Interface.h from the partial CIT files app/lcu/src/app*.cit.

Example:

> cd app/lcu/src

> make all

 . . . ’CIT’ done

 . . . ’CDT’ done

Include file ’../include/appMotorInterface.h’ done

 . . . ’include files’ done

 ...

== Building executable: ../bin/app

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 21 of 81

 . . . ’all’ done
>

Note: The final CDT and CIT files are deleted by the Makefile. Remember to perform the modifications in the ./src directory.

2.3.8 Implementation Rules for the Command Handlers

As stated in the rules applying to a Software Device, the behaviour of each command is implemented in a Command Handler. This handler must show the 2 ACI and API interfaces:

• ACI function: the ACI function name is built on the following scheme:

      ccsCOMPL_STAT Iapp<Devtype><Entry>
                               ( ... , ccsERROR *error )

It is responsible for parsing the command parameters, invoking the API function and building the reply buffer as defined in the CDT entry of this command.

• AP I function: the API function name is built on the following scheme:

      ccsCOMPL_STAT app<Devtype><Entry>
                               ( ... , ccsERROR *error )

It is the core implementation of the behaviour of the command. It must be callable from another application. It receives application specific parameters and the error stack pointer, and returns the completion status.

2.3.9 Hook functions

A hook function is implementing an additional behaviour. Four kinds of hooks are supported:

• Constructors/Destructors: One application specific constructor and one application specific destructor per device name, resp. device type may be implemented. These functions will be invoked according to the following scheme:

• At boot time, the object constructors will be invoked as depicted in the following Sequence Diagram.

: lsf Init All

: lsf SERVER_DATA : lsf CONTROL_DATA : lsfDEVICE_DATA : lsfDEVICE_ENTRY

lsfServerConstructor( ) lsfControlConstructor( )

lsf<devType>Constructor( )

app<devName>Constructor( ) app<devType>Constructor( )

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25

22 of 81

The application specific constructors have the prototype:

ccsCOMPL_STAT app<devType>Constructor ( IN  void       *devData,

                                  IN  const char *devName,

                                  OUT ccsERROR   *error )
ccsCOMPL_STAT app<devName>Constructor ( IN  void       *devData,

                                  IN  const char *devName,

                                  OUT ccsERROR   *error )

• At exit time, the object destructors will be invoked as depicted in the following Sequence

Diagram.

: EXIT

: lsf SERVER_DATA : lsf CONTROL_DATA : lsfDEVICE_DATA : lsfDEVICE_ENTRY lsfServerDestructor( ) lsfControlDestructor( ) lsf<devType>Destructor( ) app<devName>Destructor( ) app<devType>Destructor( )

The application specific destructors have the prototype:

ccsCOMPL_STAT app<devType>Destructor  ( IN  void *devData )
ccsCOMPL_STAT app<devName>Destructor  ( IN  void *devData )

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 23 of 81

• Standard Commands: 3 hooks per standard command may be implemented. The hook function names must follow the prototype convention:

ccsCOMPL_STAT appStd<Command><Type>Hook ( IN  lsfSERVER_DATA *serverData,
                                          OUT ccsERROR       *error )

where Command is the name of the command (Init, Standby, Online, Stop, Off, Exit,

Selftest, Test),

and Type is the hook type (Pro, Mid, Epi) resp. for the prologue, the intermediate and the epilogue additional statements. The intermediate hook is invoked only together with at least one sub- Software Device and one Hardware Device. The hooks are located in the file appStdHooks.c. They do not need any prototype declaration.

: User

: Com m and Interpreter

INIT : Com m and

Handler

: lsfDEVICE_DATA : Hardware Device : Software Device

INIT

OK

IlsfInit( )

SUCCESS

*[all HW devices]:devInit( ) lsfInit( )

init lsfStop( )

*[all SW devices]:devInit( ) forward INIT com m and userStdInitP roH ook()

userStdInitMidHook()

userStdInitEpiHook()

[I/O signal devices]:userSignalInitHook()

• Signals Initialization hook: a dedicated hook might be implemented that allows the proper setting of the signals at initialization, thus setting the sub-system in a known state. The hook function has the following prototype:

ccsCOMPL_STAT appSignalInitHook ( IN  lsfSIGNAL_DATA *signalData,
                                  IN  const char     *signalName,
                                  OUT ccsERROR       *error )

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

24 of 81

• Task device hooks: One hook function per task device must be implemented, additional 2 hooks are optional.

The mandatory hook function implements the core of the task and the prototype is:

ccsCOMPL_STAT app<TaskDevName> ( IN  lsfTASKDEV_DATA *taskDevData,

                                 IN  const char      *taskDevName,

                                 OUT ccsERROR        *error ) where TaskDevName is the name of the task device (starting with upper case).

The 2 additional hooks are invoked whenever implemented before entering the loop, resp. when terminating. The hook functions must be prototyped:

ccsCOMPL_STAT app<TaskDevName>ProHook ( IN  lsfTASKDEV_DATA *taskDevData,

                                        IN  const char      *taskDevName,

                                        OUT ccsERROR        *error ) resp.

ccsCOMPL_STAT app<TaskDevName>EpiHook ( IN  lsfTASKDEV_DATA *taskDevData,

                                        IN  const char      *taskDevName,

                                        OUT ccsERROR        *error )

2.3.10 Miscellaneous

• Adding source files: There is no limitation in adding new source or include files to the module repository. These files must be listed in the makefile either under the list app_OBJECTS for a source file, or under INCLUDES for an include file to be installed, see also Makefile(5).

Last modified: Thu Oct 26 14:23:30 METDST 2000

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 25 of 81

3 Refer ence

In this section, the man-pages of the utilities, objects anf database classes are provided. The public include files are appended.

Utility Code Database Class Include File

lsf(1)  lsfTemplate.db lsfDefines.h
lsfCreate(1)
lsfConfig(1)
lsfBackup(1)
 lsfServer(3) lsfDB_SERVER(5) lsfServer.h
 lsfStandard(3)

 lsfHandleBreak(3)
                    lsfHandleKill(3)

 lsfControl(3) lsfDB_CONTROL(5)
                                        lsfDB_DATA(5) lsfControl.h
 lsfDevice(3) lsfDB_DEVICE(5) lsfDevice.h
 lsfSignal(3) lsfDB_SIGNAL(5) lsfSignal.h
 lsfMotor(3) lsfDB_MOTOR(5) lsfMotor.h
 lsfSerial(3) lsfDB_SERIAL(5) lsfSerial.h
 lsfTaskDev(3) lsfDB_TASKDEV(5) lsfTaskDev.h
 lsfSoftDev(3) lsfDB_SOFTDEV(5) lsfSoftDev.h

Last modified: Fri Aug 11 08:21:18 METDST 2000

3.1 Utilities

3.1.1 lsf(1)

NAME

     lsf - LCU Server Framework

SYNOP SIS

     > lsfCreate <modName>
     > emacs <modName>/ws/config/<modName>.cfg
     > lsfConfig <modName>
     > emacs <modName>/lcu/src/<modName>Public.cdt
     > cd <modName>/ws/src  ; make clean all man install ; cd -
     > cd <modName>/lcu/src ; make clean all man install ; cd -

DESCRIP TION

     lsf is a framework for developing LCU Server Applications. It
     consists of a WS part dedicated to the generation and
     configuration/customization  of the target application module and
     of a LCU part providing the application architecture and implementing
     the minimum behaviour for the standard commands.

     1 - The WS part:
       1.1 Script lsfCreate(1): creates a software module compliant with
           the VLT Standards from a template.
       1.2 Script lsfConfig(1): customizes the software module according

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

26 of 81

           to the software device description file.

       1.3 The description file: is an ASCII file containing the definition

           of all devices (hardware and software) to be controlled by the

           application and of all the commands to be accepted by the

           application.

           The devices are grouped in 7 types:

           - signal (analog or digital) based on VLT AIO resp. ACRO boards

           - motor (all types as supported by MCM)

           - serial communication link (RS232, RS422 or RS485) based on

             VxWorks tyCo driver or VLT ISER8 board.

           - software device (any lsf-based application to be controlled

             from this software device)

           - tasks (any periodic background process)

           - encoder [not supported yet]

           - network [not supported yet]

           The commands are grouped in 3 types:

           - public for normal operations

           - maintenance for software/hardware verification work

           - test with restricted access to technical staff

       1.4 The database is a partial mirror (based on the scan system) of

           the LCU database

     2 - The LCU part:

       2.1 Code: the binary code lsf is to be downloaded to the LCU prior

           to loading the application software. It implements the minimum

           behaviour of the supported devices for the standard commands.

       2.2 Database: the database architecture is provided.

           The device classes may be customized by sub-classing

           to the needs of the application.

     3 - Creating a new application

       The creation of a new module is made by the utility lsfCreate.

       It receives the name of the module <mod> as argument.

       The module name shall not be registered in the CMM archive.

       Example:

         From the parent directory of <mod>

         > lsfCreate mod

         Retrieving module ’lsftpl’ ... done

         Renaming module ’lsftpl’ to ’mod’ ... done

         Renaming all files with prefix ’mod’ ... done

         Replacing pattern ’lsftpl’ by ’mod’ ... done

         1.24u 49.41s 1:59.60 42.3%

         >

     4 - Customizing the software device

       The customizatin of a new module is made by the utility lsfConfig.

       The file <mod>/ws/config/<mod>.cfg must be edited and its content

       modified to the needs of the application <mod>.

       LSF.MODULE.NAME     <mod>

       LSF.DEVICE.NUM      << the number of devices to be controlled >>

       Mandatory for each device <d>:

       LSF.DEVICEd.NAME    << the name of the device,

                              it defines the name of a database point >>

       LSF.DEVICEd.TYPE    << the type of the device:

                              analog, digital: for signals

                              serial: for serial communication links

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 27 of 81

                              motor: for motorized axis
                              taskdev: for a periodic background process
                              softdev: for a sub-software device,
                              it defines the type of control, and the
                              associated database class >>
       The following 2 entries are optional:
       LSF.DEVICEd.CLASS   << the specialized database class name mapping
                              the device. For motors, the motor class
                              name (e.g. motDVAMI) >>
       LSF.DEVICEd.PARAM   << for motors only, the number of entries in
                              the named position (P), named speed (V),
                              initialization sequence (I) and unit conversion
                              methods (U), following the syntax:
                              "P <p>,V <v>,I <i>,U <u>" >>

       LSF.COMMAND.NUM     << the number of commands to be accepted,
                              in addition to the standard commands >>

       Mandatory for each command <c>:
       LSF.COMMANDc.NAME   << the name of the command as specified for
                              the CDT (7 char.) >>
       LSF.COMMANDc.DEST   << signal, motor, serial, softdev or server
                              where "server" indicates that the command
                              is to be processed internally (no device
                              interaction).
                              NB: task devices do not process commands >>
       LSF.COMMANDc.GROUP  PUBLIC, MAINTENANCE or TEST

       LSF.COMMANDc.ENTRY  << API Funtion name <Fct> following the rule:
                              <mod><Devtype><Fct>()
                              The ACI function name is built automatically
                              as I<mod><Devtype><Fct>() in the corresponding
                              CIT file. Where <Devtype> is the destination
                              device type (e.g. "Signal") >>
       LSF.COMMANDc.INVOKE TASK or FUNCTION
       LSF.COMMANDc.OPTION << for TASK invocation only, the parameters
                              as for the CIT entries without REGISTER >>

       Example:
         From the parent directory of <mod>
         > lsfConfig mod
         Parse file ’mod/ws/config/mod.cfg’ ... done
         Found 11 devices:
              2 Motor    : M1 M2
              8 Signal   : AI1 AO3 AO4 AI8 DO1 DI2 DI3 DO4
              1 Taskdev  : bgTask
         Found 6 PUBLIC commands:
              1 Motor    : MOVEA
              4 Signal   : RASIG WASIG RDSIG WDSIG
              1 Server   : MAINCMD
         Found 0 MAINTENANCE command
         Found 0 TEST command
         Generate ’mod/ws/config/mod.dbcfg’ ... done
         Generate ’mod/lcu/include/modDeviceList.h’ ... done
         Generate ’mod/lcu/dbl/mod.db’ ... done
         Generate ’mod/lcu/src/Makefile’ ... done
         Generate ’mod/lcu/src/modPublic.cdt’ ... done
         Generate ’mod/lcu/src/modServer.cit’ ... done
         Generate ’mod/lcu/src/modMotor.cit’ ... done
         Generate ’mod/lcu/src/modSignal.cit’ ... done

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

28 of 81

         Move unused files to ./lcu/tmp ... done

         Add change log entry ... done

         >>> Remember to edit the CDT files ...

         Module configuration for ’mod’ ... done

         >

     5 - Application specific code

       The following files must be edited:

       - <mod>/lcu/src/<mod>*.cdt: describe all the command parameters

         and reply

       - <mod>/lcu/dbl/<mod>DB_DEVICE.class: define the sub-classes

         of lsfDB_DEVICE (or derived) which have been referenced in the

         device description file <mod>/ws/config/<mod>.cfg

       - <mod>/lcu/src/<mod><Devtype>.c: for each referenced device type

         <devtype>, implement the API functions

       - <mod>/lcu/include/<mod><Devtype>.h: declare the API function

         prototypes

       - <mod>/lcu/src/<mod><Devtype>Interface.c: for each command,  in

         implement the ACI functions

     6a - Extend the behaviour of the standard commands

       For each of the standard commands, up to 3 hook functions might be

       defined following the prototype:

         ccsCOMPL_STAT <mod>Std<cmd><typ>Hook

                                      ( IN  lsfCONTROL_DATA *controlData,

                                        OUT ccsERROR        *error)

       where

         <mod> is the module name,

         <cmd> is the standard command name (Init, Online etc...)

         <typ> is the hook index (Pro,Mid,Epi)

            Pro: hook is invoked when entering the method,

            Mid: hook is invoked between Software and Hardware device control

            Epi: hook is invoked before leaving the method.

       The first (Pro) and last (Epi) are called from within the standard

       object regardless on the number of devices. The middle hook (Mid) is

       only invoked from within this object.

       The prototypes to these functions do not need be declared. The hook

       functions shall be located in <mod>/lcu/src/<mod>Standard.c

       In addition, for the signals only the optional hook function

         ccsCOMPL_STAT <mod>SignalInitHook

                                      ( IN  lsfSIGNAL_DATA *signalData,

                                        IN  const char     *signalName,

                                        OUT ccsERROR       *error )

         might be implemented in <mod>/lcu/src/<mod>Signal.c

     6b - Extend the behaviour of the device constructors/destructors

       For each device type and each device, a specific additional constructor

       resp. destructor might be implemented. These functions must be defined

       following the prototype:

         ccsCOMPL_STAT <mod><devName>Constructor ( IN  void       *devData,

                                                   IN  const char *devName,

                                                   OUT ccsERROR   *error)

         void          <mod><devName>Destructor  ( IN  void       *devData )

       The user specific constructors are invoked at completion of the

       standard constructor for each device type, then for each device of

       this type;

       the user specific destructors for each device of each type followed

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 29 of 81

       by theuser specific destructor for this device type are invoked
       prior to the standard destructor.

     7 - Task devices
       The task devices are scheduled according to the state of the
       Software Device and is configurable in the database.
       The periodic loop associated to a task device is implemented within
       the framework. The core function of the task is mandatory and must
       be prototyped:
         ccsCOMPL_STAT <mod><Devname> ( IN  lsfTASKDEV_DATA *taskDevData,
                                        IN  const char       *taskDevName,
                                        OUT ccsERROR         *error )
       Two optional hooks might be implemented that are invoked when
       starting resp. when terminating the task.
       The function name syntax follows:
         ccsCOMPL_STAT <mod><Devname>ProHook() for the prologue function, and
         ccsCOMPL_STAT <mod><Devname>EpiHook() for the epilogue function,
           same parameters as the core function.

       The method lsfTaskDevTrigger() is provided that triggers
       asynchronously the task, if running.

     8 - Building the code
       On both <mod>/ws/src and <mod>/lcu/src, invoke:
         make clean all man install

     9 - Building the environments
       The instantiation of the database point associated to the Software
       Device is realized from within the file:
         $VLTDATA/ENVIRONMENTS/<env>/dbl/DATABASE.db

         #define <mod>DB_ROOT "<< database absolute path >>"
         #include "<mod>.db"

       On the LCU environment, the file ’bootScript’ shall be updated
       that contains the modules: lcc, cai, scan, too, mcm, lsf and <mod>
       The file ’devicesFile’ shall be updated as well with the entry
       corresponding to the new Software Device:
         "<mod>" "<mod>Server" 1 0 0 1
       NB: any Software Device to be controlled by another Software Device
           MUST NOT be declared in this list.
     10 - Database configuration file
       The default database configuration file <mod>/ws/config/<mod>.dbcfg
       shall be updated to store the complete final device configuration.
       The backup of the database configuration is made by the utility
       lsfConfig.

       Example:
         From the directory of <mod>/ws/config
         > lsfBackup -e <lcuEnv> -m mod
         Generating input file ’./mod.inp’ ... done
         Performing database backup into  ’./mod.dbcfg’ ... done
         1.24u 49.41s 1:59.60 42.3%
         >

SEE ALSO

     lsfCreate(1), lsfConfig(1), lsfBackup(1)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

30 of 81

3.1.2 lsfCreate(1)

NAME

     lsfCreate - Create a new module from lsftpl template

SYNOP SIS

     lsfCreate [-f] <modName>

DESCRIP TION

     This script creates a module directory <modName> from the

     template module ’lsftpl’.

     It checks that the new module is not already existing in the

     CMM Archive.

     It renames all files with the new prefix.

     It replaces all occurences of ’lsftpl’ by ’modName’ in lower

     and upper case.

     Finally it creates the file <modName>/ChangeLog with one entry.

     Options:

     -f : the module is created anyway

          the existing module ’modName’ is renamed ’modName-old’

          the module is created even if already in the CMM archive

ENVIRONMENT

     CMM

RETURN VALUES

     0 on SUCCESS

     1 on Failure

CAUTIONS

     The module is not created if it already exists under the CMM archive

     or if the directory ’modName’ already exists. Option -f bypasses these

     checks.

EXAMP LES

     > lsfCreate app

     Copying template module ’lsftpl’ to ./app ... done

     Renaming all files with prefix ’app’ ... done

     Replacing pattern ’lsftpl’ by ’app’ ... done

     1.24u 49.41s 1:59.60 42.3%

     Module creation ’app’ ... done

     >

SEE ALSO

     lsf(1), cmmCopy

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

33 of 81

3.1.4 lsfBackup(1)

NAME

     lsfBackup - Save LCU database configuration into file

SYNOP SIS

     lsfBackup -e <lcuEnv> -m <modName> [-o <fileName>]

DESCRIP TION

     This script saves the content of the LCU database to a file.

     It generates a ".dbcfg" type file containing all the configuration

     attributes of the module.

     Arguments:

     lcuEnv  : LCU environment name

     modName : module name (alias of the database top point)

     fileName: output file name (default to "./<modName>.dbcfg"

FILES

ENVIRONMENT

RETURN VALUES

     0 on SUCCESS

     1 on Failure

CAUTIONS

EXAMP LES

     > lsfBackup -e lcuEnv -m app

     Generating input file ’./app.inp’ ... done

     Performing database backup into  ’./app.dbcfg’ ... done

     1.24u 49.41s 1:59.60 42.3%

     >

SEE ALSO

     dbBackup

BUGS

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 34 of 81

3.2 Code

3.2.1 lsfServer(3)

NAME

   lsfServer - Top level control of the application

SYNOP SIS

     #include "lsfServer.h"

DESCRIP TION

     This class provides the methods for the handling of the server process.

P UBLIC METHODS

     ccsCOMPL_STAT lsfInitAll
                        ( IN  const char      *swdName,
                          OUT lsfSERVER_DATA **pServerData )
         This method is the constructor of the application server <swdName>.
         It shall be invoked at boot time from the bootScript(5) as part
         of the application file <swdName>.boot(3).
         It receives the address of the pointer to the application global
         data <pServerData>.
         The method loads the database from the file <swdName>.dbcfg
         located under VLTROOT/config or $INTROOT/config.
         It invokes then the server constructor and finally spawns the
         command interpreter with the associated CDT and CIT files.

     vltLOGICAL    lsfServerGetInit
                        ( IN lsfSERVER_DATA *serverData )
         This method returns the initialization status of the device.

     vltLOGICAL    lsfServerGetSim
                        ( IN  lsfSERVER_DATA *serverData )
         This method returns the simulation status of the device.
     lccDEV_MODE   lsfServerGetState
                        ( IN  lsfSERVER_DATA *serverData )
     const char   *lsfServerGetStateName
                        ( IN  lsfSERVER_DATA *serverData )
         These methods return the state and state’s name name of the device.

     vltINT32      lsfServerGetSubState
                        ( IN  lsfSERVER_DATA *serverData )
     const char   *lsfServerGetSubStateName
                        ( IN  lsfSERVER_DATA *serverData )
         These methods return the subState and subState’s name of the device.

     ccsCOMPL_STAT lsfServerCheckOnline
                        ( IN  lsfSERVER_DATA *serverData,
                          OUT vltLOGICAL     *online,
                          OUT ccsERROR       *error )
         This method returns the flag <online> indicating if the device
         is in state ONLINE when True.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

35 of 81

     lsfSERVER_DATA *lsfServerGetGlobalData

                        ( IN  const char     *swdName,

                          OUT ccsERROR       *error )

         This method returns the pointer to the global data structure of

         the device.

     ccsCOMPL_STAT lsfServerGetSwDeviceName

                        ( OUT char           *swdName,

                          OUT ccsERROR       *error )

         This method returns the name of the device from the task name of

         the commmand interpreter process.

     vltLOGICAL    lsfServerIsALccDevice

                        ( IN  lsfSERVER_DATA *serverData )

         This method returns the flag indicating if the device is registered

         in the LCC Device Table.

         Any Software Device controlled by another Software Device

         must NOT be registered in LCC.

P ROTECTED METHODS

     void          lsfServerDestructor

                        ( IN  lsfSERVER_DATA **pServerData )

         This method is the object destructor. All resources are released.

     void          lsfServerGetHooks

                        ( IN  lsfSERVER_DATA  *serverData )

         This method resolves the addresses of all existing hook functions

         provided by the application. It is invoked once at Init time.

         The function entry points are retrieved from the global

         symbol table.

     ccsCOMPL_STAT lsfServerCallHook

                        ( IN  lsfSERVER_DATA  *serverData,

                          IN  lsfHOOKFUNC_IDX  cmd,

                          IN  lsfHOOKTYPE_IDX  typ,

                          OUT ccsERROR        *error )

         This method resolves the hook function <typ> [Pro,Mid or Epi]

         associated to the command indexed by <cmd>, if resolved.

     ccsCOMPL_STAT lsfServerReadConfig

                        ( IN  lsfSERVER_DATA *serverData,

                          OUT ccsERROR       *error )

         This method reads the device configuration from the database.

     ccsCOMPL_STAT lsfServerSetInit

                        ( IN  lsfSERVER_DATA *serverData,

                          IN  vltLOGICAL      value,

                          OUT ccsERROR       *error )

         These methods set/return the initialization status of the device.

     ccsCOMPL_STAT lsfServerSetSim

                        ( IN  lsfSERVER_DATA *serverData,

                          IN  vltLOGICAL      value,

                          OUT ccsERROR       *error )

         This method sets the simulation status of the device.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 36 of 81

     ccsCOMPL_STAT lsfServerTakeInitSem
                        ( IN  lsfSERVER_DATA *serverData )
     void          lsfServerGiveInitSem
                        ( IN  lsfSERVER_DATA *serverData )
         These methods control the initialization semaphore associated
         to the device. It prevents multiple invocation.

     ccsCOMPL_STAT lsfServerTakeCmdSem
                        ( IN  lsfSERVER_DATA *serverData )
     void          lsfServerGiveCmdSem
                        ( IN  lsfSERVER_DATA *serverData )
         These methods control the command semaphore associated
         to the device. It prevents multiple invocation.

     void          lsfServerWakeupMonitor
                        ( IN lsfSERVER_DATA *serverData  )
         This method triggers the monitor task for state update

     vltINT32      lsfServerGetCmdTimeout
                        ( IN  lsfSERVER_DATA *serverData )
     void          lsfServerSetCmdTimeout
                        ( IN  lsfSERVER_DATA *serverData,
                          IN  vltINT32        timeout )
         These methods set/get the timeout value associated to the commands.

     ccsCOMPL_STAT lsfServerSwitchState
                        ( IN  lsfSERVER_DATA *serverData,
                          IN  lccDEV_MODE     newDevState,
                          OUT ccsERROR       *error )
         This method instructs LCC of the new state <newDevState> of the
         device.

     int           lsfStartupTask
                        ( IN  char           *name,
                          IN  vltINT32        priority,
                          IN  vltINT32        stackSize,
                          IN  FUNCPTR         entryPoint,
                          IN  void           *param,
                          OUT ccsERROR       *error )
         This method spawns the task <name> with the appropiate parameters,
         and checks the task has synchronized with the caller. The task entry
         function must comply with the prototype lsfTASK_FUNCTION.
           typedef void lsfTASK_FUNCTION ( IN void          *parameter,
                                           IN SEM_ID        *syncSem,
                                           IN ccsCOMPL_STAT *status )
         The first argument is application dependent. The semaphore <syncSem>
         must be given by the task within 1 second, and the task status
         <status> shall be set accordingly to SUCCESS or FAILURE.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

37 of 81

P RIVATE METHODS

     static ccsCOMPL_STAT lsfServerUpdateState

                        ( IN  lsfSERVER_DATA  *serverData,

                          OUT ccsERROR        *error )

     static ccsCOMPL_STAT lsfServerUpdateSubState

                        ( IN  lsfSERVER_DATA  *serverData,

                          OUT ccsERROR        *error )

         These 2 methods are responsible for updating the state and subState

         of the device. They query the individual states and subStates of all

         registered devices.

         The device state is set to the lower state of the devices.

         The subState is set to :

         - lsfSUBSTATE_ERROR if any device is in that subState.

         - lsfSUBSTATE_INITIALIZING if any device is in that subState.

         - lsfSUBSTATE_IDLE  if all devices are in that subState

         - lsfSUBSTATE_ACTIVE if any device is not lsfSUBSTATE_IDLE and

              the device subState is not lsfSUBSTATE_IDLE

         - lsfSUBSTATE_<ACTION> if a device is in that subState and

              the device subState is lsfSUBSTATE_IDLE

         The following subStates are dedicated:

         - lsfSUBSTATE_MOVING for a motor when moving

         - lsfSUBSTATE_MONITORING for a device monitoring a piece of hardware

         In addition, the subState lsfSUBSTATE_TIMEOUT indicates a timeout

         occured.

         Both lsfSUBSTATE_TIMEOUT and lsfSUBSTATE_ERROR are transient

         subStates that reset to lsfSUBSTATE_IDLE with the next action.

     static ccsCOMPL_STAT lsfServerInitDb

                        ( IN  const char      *swdName,

                          OUT ccsERROR        *error )

         This method is invoked at boot time by lsfInitAll(). It restores

         the content of the device database branch from the file

         <swdName>.dbcfg located under $VLTROOT/config or $INTROOT/config.

     static void lsfServerMonitor

                        ( IN  void            *pData,

                          IN  SEM_ID          *pSyncSem,

                          IN  ccsCOMPL_STAT   *pStatus )

         This method is invoked as a task (see lsfStartupTask) at construction

         time. It is responsible for updating the device global state and

         subState at the given rate (see lsfSERVER(5)).

         Note: be aware that a high polling rate is CPU consuming and might

         impact on the overall behaviour of the system.

     static ccsCOMPL_STAT lsfServerConstructor

                        ( IN  const char      *swdName,

                          OUT lsfSERVER_DATA **pServerData,

                          OUT ccsERROR        *error )

         This method is the constructor of the software device. It invokes

         the control contructor (see lsfControl(3)) and spawns the monitor.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 38 of 81

P RIVATE DATA MEMBERS

     typedef struct
     {
       void        *ctrlData;     Ptr to Control Data structure
       lccDEV_MODE  state;        Module state
       vltINT32     subState;     Module sub-state
       vltLOGICAL   init;         True if initialized
       vltLOGICAL   simulation;   True if in simulation
       vltINT32     numDevices;   number of controlled devices (registered)

       SEM_ID       cmdSem;       semaphore for sending commands
       vltINT32     cmdTimeout;   timeout for sending commands
       SEM_ID       initSem;      semaphore for init command
       vltLOGICAL   lccDevice;    SW device is a LCC device
       int          monTid;       Monitoring Task Id
       SEM_ID       monSem;       semaphore for monitor task period
       int          monPeriod;    Monitoring Task Period (ticks)
       ccsERROR     error;        error stack for cmdInit()

       char        *attrTable;    cai DB attribute table

       vltBYTES20   swdName;      Name of the SW device
       void        *fctHook[8][3]; Hook function addresses
     } lsfSERVER_DATA;

FILES

     $INTROOT/config/<modName>.dbcfg

DATABASE

     The class lsfDB_SERVER is a sub-class of lsfDB_SOFTDEV.
     It is partially mapped by the data structure lsfSERVER_DATA.

SEE ALSO

     lsfControl(3), lsfDevice(3), lsfDB_DEVICE(5)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

39 of 81

3.2.2 lsfStandard(3)

NAME

     lsfStandard - Standard commands

SYNOP SIS

     #include "lsfStandard.h"

DESCRIP TION

     This class provides the methods implementing the high level default

     behaviour of the standard commands.

     For each of the standard commands, up to 3 hook functions might be

     defined following the syntax:

       <mod>Std<cmd><typ>Hook(lsfSERVER_DATA *serverData, ccsERROR *error)

     where

       <mod> is the module name,

       <cmd> is the standard command name (Init, Online etc...)

       <typ> is the hook index (Pro,Mid,Epi)

            Pro: hook is invoked when entering the method,

            Mid: hook is invoked between Software and Hardware device control

            Epi: hook is invoked before leaving the method.

     The first (Pro) and last (Epi) are called regardless on the number

     of devices. The middle hook (Mid) is only invoked from within the control

     object.

P UBLIC METHODS

     ccsCOMPL_STAT lsfStdInit

     ccsCOMPL_STAT lsfStdStandby

     ccsCOMPL_STAT lsfStdOnline

     ccsCOMPL_STAT lsfStdStop

     ccsCOMPL_STAT lsfStdExit

     ccsCOMPL_STAT lsfStdStartSim

     ccsCOMPL_STAT lsfStdStopSim

     ccsCOMPL_STAT lsfStdSelfTest

     ccsCOMPL_STAT lsfStdTest

                        ( IN  lsfSERVER_DATA *serverData,

                          IN  const char     *devName,

                          OUT ccsERROR       *error )

         These methods implement the high level behaviour associated

         to the standard commands. They invoke the associated control

         method for the specified device <devName>.

         If <devName> is set to the software device name, the method

         affects all devices registered in that software device, otherwise

         the action is restricted to the one device.

         At completion, the methods update the global state accordingly.

     ccsCOMPL_STAT lsfStdGetInit

                        ( IN  lsfSERVER_DATA *serverData,

                          OUT vltLOGICAL     *init,

                          OUT ccsERROR       *error )

         This method returns the initialization status.

     ccsCOMPL_STAT lsfStdGetSimulation

                        ( IN  lsfSERVER_DATA *serverData,

                          OUT vltLOGICAL     *simulation,

                          OUT ccsERROR       *error )

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 40 of 81

         This method returns the value of the simulation flag.

     ccsCOMPL_STAT lsfStdGetVersion
                        ( OUT char           *version,
                          OUT ccsERROR       *error )
         This method returns the software version of the module LSF.

P RIVATE METHODS

     static const char *lsfCheckDevice
                        ( IN  lsfSERVER_DATA *serverData,
                          IN  const char     *devName,
                          OUT ccsERROR       *error )
         This method checks if the given device is known:
         - name of the software device or "all", it returns "all"
         - name of a controlled device, it returns the name if defined.
         - unknown name, it returns NULL.

P RIVATE DATA MEMBERS

       These methods use the data structure <serverData>.

COMMANDS

       The public methods are the API functions associated to the
       ACI for the Standard Commands.

RETURN VALUES

       SUCCESS if everything ok
       FAILURE, the error structure is updated with:
           lsfERR_DEVICE           : unknown device name or
                                     module name mismatch
           lsfERR_MULTIPLE_COMMAND : multiple invocation not allowed

SEE ALSO

     lsfServer(3)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

41 of 81

3.2.3 lsfSignalHandlers(3)

NAME

     lsfHandleBreak, lsfHandleKill - signal handler for BREAK and KILL signals

SYNOP SIS

     #include "lsfSignalHandlers.h"

     void lsfHandleKill(void);

     void lsfHandleBreak(void);

DESCRIP TION

     lsfHandleBreak() and lsfHandleKill() are the 2 signal handler methods

     installed at boot time by lsfInitAll(). These methods retrieve the

     name of the affected software device from the server task name before

     performing the corresponding actions (STOP, resp. EXIT).

RETURN VALUES

       None

SEE ALSO

       lsfStandard(3), lsfServer(3)

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 42 of 81

3.2.4 lsfControl(3)

NAME

     lsfControl - Device control

SYNOP SIS

     #include "lsfControl.h"

DESCRIP TION

     This class provides the methods dedicated to the control
     of the devices. It is driven by the deviceTable. This table is read
     at init time.
     For each of the standard commands, the associated control method
     invokes the device methods for each type of device assuming devices of
     that type are registered and not ignored.
     First the sub-software devices are invoked, then the hardware
     devices whereby the digital and analogue signals are processed first,
     followed by the motors.
     For each of the standard commands, up to 3 hook functions might be
     defined following the syntax:
       <mod>Std<cmd><typ>Hook(lsfCONTROL_DATA *controlData, ccsERROR *error)
     where
       <mod> is the module name,
       <cmd> is the standard command name (Init, Online etc...)
       <typ> is the hook index (Pro,Mid,Epi)
            Pro: hook is invoked when entering the method,
            Mid: hook is invoked between Software and Hardware device control
            Epi: hook is invoked before leaving the method.
     The first (Pro) and last (Epi) are called from within the standard
     object regardless on the number of devices. The middle hook (Mid) is
     only invoked from within this object.

P ROTECTED METHODS

     ccsCOMPL_STAT lsfControlConstructor
                           ( IN  const char      *swdName,
                             IN  lsfDEVICE_DATA  *serverData,
                             OUT ccsERROR        *error )
         This method is the object constructor. It invokes the constructors
         of all devices registered in the device table.
     void lsfControlDestructor
                           ( IN lsfDEVICE_DATA *serverData )
         This method is the object destructor. It invokes the destructors
         of all registered devices. All resources are released.
     const char *lsfControlGetSwdName
                           ( IN  void *pData )
         This method returns the name of the software device (= module name)
     void *lsfControlGetDevData
                           ( IN lsfCONTROL_DATA *controlData,
                             IN int devType )
         This method returns a pointer to the device data structure
         of the given device type.
     int lsfControlGetDevType
                           ( IN  lsfCONTROL_DATA *controlData,
                             IN  const char      *devName )
         This method returns the type of the given device.
     int lsfControlGetDevNamesOfType

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

43 of 81

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  int              devType,

                             IN  const char      *devNames[] )

         This method returns the number of devices of the given type.

         The array <devNames[]> contains the names of all the matching

         devices.

     ccsCOMPL_STAT lsfControlInit

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error)

     ccsCOMPL_STAT lsfControlStandby

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

     ccsCOMPL_STAT lsfControlOnline

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

     ccsCOMPL_STAT lsfControlStop

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error)

     ccsCOMPL_STAT lsfControlOff

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error)

     ccsCOMPL_STAT lsfControlExit

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

     ccsCOMPL_STAT lsfControlSimulat

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

     ccsCOMPL_STAT lsfControlStopsim

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

     ccsCOMPL_STAT lsfControlSelftest

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

     ccsCOMPL_STAT lsfControlTest

                           ( IN  lsfCONTROL_DATA *controlData,

                             IN  const char      *devName,

                             OUT ccsERROR        *error )

         These methods perform the actions corresponding to the standard

         behaviour.

P RIVATE METHODS

     static int lsfDecodeDeviceType

                           (char *type)

         This method returns the associated device type associated to

         the device type name.

     static ccsCOMPL_STAT lsfControlReadDevTbl

                           ( IN  lsfCONTROL_DATA *controlData,

                             OUT ccsERROR        *error )

         This method reads the database attribute control:deviceTable

         and sets the private data member <deviceTable>.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 44 of 81

P RIVATE DATA MEMBERS

     The data structure lsfCONTROL_ENTRY maps the database attribute
     :control.deviceTable.
     typedef struct
     {
       vltBYTES20 name;                 Name of the device
       vltINT32   type;                 Type of the device
       vltINT32   startPhase;           Sequence order for increasing/
       vltINT32   stopPhase;              decreasing the state
       vltLOGICAL simulation;           True when device is in Simulation
       vltLOGICAL ignored;              True when device is ignored
     } lsfCONTROL_ENTRY;

     The data structure lsfCONTROL_DATA holds all the necessary information
     for the control of the devices.
     typedef struct
     {
       void             *ctrlData;      Ptr to self
       void             *srvrData;      Ptr to parent structure
       int               numDevices[lsfDEVICE_NUM_TYPES+1];
                                        Number of devices of each type
       lsfCONTROL_ENTRY *deviceTable;
                                        Device table (mirror of DB)
       lsfDEVICE_DATA   *deviceData[lsfDEVICE_NUM_TYPES+1];
                                        Device data
       char             *attrTable;     LCC cai internal
       void             *fctHook[8][3]; Hook function addresses
     } lsfCONTROL_DATA;

DATABASE

     The class lsfCONTROL is the class holding the description of the
     device. It consists of the deviceTable attribute that stores the
     description of each device to be controlled:
         vltBYTES20 name;               Name of the device
         vltBYTES20 type;               Type of the device
         vltINT32   startPhase;         Sequence order for increasing/
         vltINT32   stopPhase;            decreasing the state
         vltLOGICAL simulation;         Device is in Simulation
         vltLOGICAL ignored;            Device is ignored
     For each kind of device a point is instanciated from the class lsfDEVICE
     that holds the information of that kind of devices (state, subState
     etc...). These points are instanciated dynamically at build time
     depending on the number of devices of a kind.

RETURN VALUES

     The control sequence is broken on the first failure.
     The method returns FAILURE and an error is logged.

CAUTIONS

     Start/Stop Phase handling mechanism is not yet implemented.

SEE ALSO

     lsfCONTROL(5)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

45 of 81

3.2.5 lsfDevice(3)

NAME

     lsfDevice - Common device handling methods

SYNOP SIS

     #include "lsfDevice.h"

DESCRIP TION

     This class provides methods dedicated to the handling of devices.

     The allows other objects to query device private information and

     to set the device state/subState.

P UBLIC METHODS

     vltLOGICAL    lsfDeviceIsDefined   ( IN  void       *pData,

                                          IN  const char *devName );

     vltLOGICAL    lsfDeviceIsIgnored   ( IN  void       *pData,

                                          IN  const char *devName );

     vltLOGICAL    lsfDeviceIsSimulated ( IN  void       *pData,

                                          IN  const char *devName );

     vltLOGICAL    lsfDeviceIsInState   ( IN  void       *pData,

                                          IN  vltINT32    state );

         These 4 methods query the device status.

P ROTECTED METHODS

     ccsCOMPL_STAT lsfDeviceSetStatus   ( IN  void       *pData,

                                          IN  vltINT32    devIdx,

                                          IN  vltINT32    state,

                                          IN  vltINT32    subState,

                                          IN  vltINT32    init,

                                          OUT ccsERROR   *error );

         This method sets the device status to the given values for:

         the <state>, the <subState> and the <init> flag.

         The index <devIdx> refers to the selected device when > 0

         or to the device group when zero.

     ccsCOMPL_STAT lsfDeviceSetState    ( IN  void       *pData,

                                          IN  vltINT32    devIdx,

                                          IN  vltINT32    state,

                                          OUT ccsERROR   *error );

         Idem dito for the <state> only.

     ccsCOMPL_STAT lsfDeviceSetSubState ( IN  void       *pData,

                                          IN  vltINT32    devIdx,

                                          IN  vltINT32    subState,

                                          OUT ccsERROR   *error );

         Idem dito for the <subState> only.

     ccsCOMPL_STAT lsfDeviceSetInit     ( IN  void       *pData,

                                          IN  vltINT32    devIdx,

                                          IN  vltLOGICAL  init,

                                          OUT ccsERROR   *error );

         Idem dito for the <init> flag only.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

48 of 81

     ccsCOMPL_STAT lsfSignalWriteDigital

                                  ( IN  lsfSIGNAL_DATA *signalData,

                                    IN  const char     *signalName,

                                    IN  vltUINT32      *value,

                                    OUT ccsERROR       *error )

         This method sets the specified digital signal <signalName>

         to the value pointed to by <value>.

         If <signalName> is NULL or "all", all output digital signals

         will be set to the values pointed to by <value> in the order

         they are registered.

P ROTECTED METHODS

     ccsCOMPL_STAT lsfSignalConstructor

                                  ( IN  const char      *swdName,

                                    IN  lsfCONTROL_DATA *controlData,

                                    IN  const char      *signalNames[],

                                    OUT ccsERROR        *error )

         This is the constructor of the signal object. It affects all the

         signals given in the list <signalNames[]> (NULL terminated).

     void          lsfSignalDestructor

                                  ( IN  lsfCONTROL_DATA *controlData )

         This method is the object destructor. All resources are released.

     ccsCOMPL_STAT lsfSignalInit

     ccsCOMPL_STAT lsfSignalStandby

     ccsCOMPL_STAT lsfSignalOnline

     ccsCOMPL_STAT lsfSignalStop

     ccsCOMPL_STAT lsfSignalOff

     ccsCOMPL_STAT lsfSignalExit

     ccsCOMPL_STAT lsfSignalSimulat

     ccsCOMPL_STAT lsfSignalStopsim

     ccsCOMPL_STAT lsfSignalSelftest

     ccsCOMPL_STAT lsfSignalTest

                                  ( IN  lsfSIGNAL_DATA *signalData,

                                    IN  const char     *signalName,

                                    OUT ccsERROR       *error )

         These methods implement the behaviour of the standard commands.

         If <signalName> is NULL, or "all" all the signals will be

         affected, otherwise only the specified one.

P RIVATE METHODS

     static ccsCOMPL_STAT lsfSignalCallHook

                                  ( IN  lsfSIGNAL_DATA *signalData,

                                    IN  const char     *signalName,

                                    IN  const char     *signalFct,

                                     OUT ccsERROR       *error )

         This method invokes the user-defined hook function

         <mod>Signal<signalFct>Hook(<signalData>,<signalName>,error).

         It is invoked at Init completion only.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 49 of 81

P RIVATE DATA MEMBERS

     The data stucture lsfSIGNAL_ENTRY is a sub-class of lsfDEVICE_ENTRY.
     typedef struct
     {
       vltINT32         state;
       vltINT32         subState;
       vltLOGICAL       init;
       vltLOGICAL       simulation;
       vltINT32         timeout;
                                    Additional data members
       ioTYPE           ioType;        Type of signal (Digital/Analog)
       ioIN_OUT         direction;     Signal direction (Input/Output)
       dbSYMADDRESS     dbAddr;        DB path to Signal point
       ioDIRADDRESS     ioAddr;        IO Direct address
     } lsfSIGNAL_ENTRY;

     The data stucture lsfSIGNAL_DATA is a sub-class of lsfDEVICE_DATA.
     typedef struct
     {
       void            *ctrlData;
       void            *userData;
       vltINT32         state;
       vltINT32         subState;
       vltLOGICAL       init;
       vltLOGICAL       simulation;
       vltINT32         timeout;
       vltINT32         numSignals;                    Number of signals

       vltBYTES20       *signalNames;                  Signal names
                                                      (dynamic allocated)
       char             *attrTable[lsfMAX_DEVICES+1];
       lsfSIGNAL_ENTRY  *signalTable[lsfMAX_DEVICES];  Signal data
     } lsfSIGNAL_DATA;

DATABASE

     The class lsfDB_SIGNAL is a sub-class of lsfDB_DEVICE.
     It is partially mapped by the data structure lsfSIGNAL_ENTRY.
     Each signal is represented in the database by a point under the
     main signal point :control:signal, which is partially mapped
     by the data structure lsfSIGNAL_DATA.
     The 2 sub-classes lsfDB_ANALOG and lsfDB_DIGITAL are specialized classes
     for Analogue, resp. Digital signals. They are instanciating the LCC
     classes lccANALOG_SIGNAL and lccDIGITAL_SIGNAL resp.

SEE ALSO

     lsfDB_SIGNAL(5)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

50 of 81

3.2.7 lsfMotor(3)

NAME

     lsfMotor - Control motors

SYNOP SIS

     #include "lsfMotor.h"

DESCRIP TION

     This class provides the methods for the control of motors.

     It implements the default behaviour for all the standard commands.

     In addition, it offers 2 methods for performing absolute motions

     on one or all motors in parallel.

P UBLIC METHODS

     vltINT32 lsfMotorGetState    ( IN  lsfMOTOR_DATA *motorData,

                                    IN  const char    *motorName )

     vltINT32 lsfMotorGetSubState ( IN  lsfMOTOR_DATA *motorData,

                                    IN  const char    *motorName )

         These 2 methods return the state, resp. sub-state of the motors

         specified by <motorName>.

     ccsCOMPL_STAT lsfMotorMoveAbs

                                  ( IN  lsfMOTOR_DATA *motorData,

                                    IN  const char    *motorName,

                                    IN  vltINT32       target[],

                                    IN  const char    *unit[],

                                    IN  vltLOGICAL     wait,

                                    OUT ccsERROR      *error )

         This methods initiates an absolute motion to the position

         <target> for all the motors specified by <motorName>. The

         position unit is specified by <unit> in the corresponding order.

         The flag <wait> indicates whether the function shall wait for

         the motion completion, or not.

     ccsCOMPL_STAT lsfMotorWaitMove

                                  ( IN  lsfMOTOR_DATA *motorData,

                                    IN  const char    *motorName,

                                    OUT char          *names[],

                                    OUT vltDOUBLE     *position,

                                    OUT char          *units[],

                                    OUT ccsERROR      *error )

         This method is based on the API function motWaitMove() that

         waits until all motors specified by <motorName> have completed

         their motion. It returns on the first error.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 51 of 81

P ROTECTED METHODS

     ccsCOMPL_STAT lsfMotorConstructor
                                  ( IN  const char      *swdName,
                                    IN  lsfCONTROL_DATA *controlData,
                                    IN  const char      *motorNames[],
                                    OUT ccsERROR        *error )
         This is the constructor of the motor object. It affects all the
         motors given in the list <motorNames[]> (NULL terminated).
     void          lsfMotorDestructor
                                  ( IN  lsfCONTROL_DATA *controlData )
         This method is the object destructor. It deinstalls all
         of all registered motors. All resources are released.

     ccsCOMPL_STAT lsfMotorInit
     ccsCOMPL_STAT lsfMotorStandby
     ccsCOMPL_STAT lsfMotorOnline
     ccsCOMPL_STAT lsfMotorStop
     ccsCOMPL_STAT lsfMotorOff
     ccsCOMPL_STAT lsfMotorExit
     ccsCOMPL_STAT lsfMotorSimulat
     ccsCOMPL_STAT lsfMotorStopsim
     ccsCOMPL_STAT lsfMotorSelftest
     ccsCOMPL_STAT lsfMotorTest   ( IN  lsfMOTOR_DATA  *motorData,
                                    IN  const char     *motorName,
                                    OUT ccsERROR       *error )
         These methods implement the behaviour of the standard commands.
         If <motorName> is NULL, or "all" all the motors will be
         affected, otherwise only the specified one.

     ccsCOMPL_STAT lsfMotorWaitInit
                                  ( IN  lsfMOTOR_DATA *motorData,
                                    IN  const char    *motorName,
                                    OUT ccsERROR      *error )
         This method is based on the API function motWaitInit() that
         waits until all motors specified by <motorName> have completed
         their initialization sequence. It returns on the first error.

     ccsCOMPL_STAT lsfMotorSetSubState
                                  ( IN  lsfMOTOR_DATA *motorData,
                                    OUT ccsERROR      *error )
         This method sets the sub-states of all registered motors as a
         function of their resp. initStatus and motionStatus.

P RIVATE DATA MEMBERS

     The data stucture lsfMOTOR_ENTRY is a sub-class of lsfDEVICE_ENTRY.
     typedef struct
     {
       vltINT32         state;
       vltINT32         subState;
       vltLOGICAL       init;
       vltLOGICAL       simulation;
       vltINT32         timeout;
                                    Additional data members
       motSTATUS       *motorStatus;   Ptr to motorStatus array
                                       from lsfMOTOR_DATA
     } lsfMOTOR_ENTRY;

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

52 of 81

     The data stucture lsfMOTOR_DATA is a sub-class of lsfDEVICE_DATA.

     typedef struct

     {

       void            *ctrlData;

       void            *userData;

       vltINT32         state;

       vltINT32         subState;

       vltLOGICAL       init;

       vltLOGICAL       simulation;

       vltINT32         timeout;

       vltINT32         numMotors;                    Number of motors

       vltBYTES20      *motorNames;                   Motor names

                                                      (dynamic allocated)

       char            *attrTable[lsfMAX_DEVICES+1];

       lsfMOTOR_ENTRY  *motorTable[lsfMAX_DEVICES];   Motor data

                                    Additional data members

       motHANDLE        motorHandle[lsfMAX_DEVICES+1]; List of motor

                                                       handles [0 terminated]

       motSTATUS       *motorStatus;                  Array of motor status

                                                      (dynamic allocated)

     } lsfMOTOR_DATA;

DATABASE

     The class lsfDB_MOTOR is a sub-class of lsfDB_DEVICE.

     It is partially mapped by the data structure lsfMOTOR_ENTRY.

     Each motor is represented in the database by a point under the

     main  warning: imsignal point :control:motor, which is partially mapped

     by the data structure lsfMOTOR_DATA.

SEE ALSO

     lsfDB_MOTOR(5)

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 53 of 81

3.2.8 lsfSerial(3)

NAME

     lsfSerial - Control serial communication links

SYNOP SIS

     #include "lsfSerial.h"

DESCRIP TION

     This class provides the methods for the control of serial
communication links. It implements the default behaviour for all
     the standard commands.

P UBLIC METHODS

     ccsCOMPL_STAT lsfSerialRead  ( IN  lsfSERIAL_DATA *serialData,
                                    IN  const char     *serialName,
                                    OUT char           *names[],
                                    OUT char           *buffer[],
                                    OUT ccsERROR       *error)
         This method reads data from the given serial communication
         link <serialName> into the buffer pointed to by <buffer>.
         If <serialName> is NULL or "all", all communication links
         will be read in the order they are registered. The names of
         devices read are returned in the array <names[]>. The data
         buffers are ordered identically.

     ccsCOMPL_STAT lsfSerialWrite ( IN  lsfSERIAL_DATA *serialData,
                                    IN  const char     *serialName,
                                    IN  char           *buffer[],
                                    OUT ccsERROR       *error )
         This method writes data pointed to by <buffer> to the given
         serial communication link <serialName>.
         If <serialName> is NULL or "all", all communication links
         will be written in the order they are registered.

P ROTECTED METHODS

     ccsCOMPL_STAT lsfSerialConstructor
                                  ( IN  const char      *swdName,
                                    IN  lsfCONTROL_DATA *controlData,
                                    IN  const char      *serialNames[],
                                    OUT ccsERROR        *error )
         This is the constructor of the serial object. It affects all the
         serials given in the list <serialNames[]> (NULL terminated).
     void          lsfSerialDestructor
                                  ( IN  lsfCONTROL_DATA *controlData )
         This method is the object destructor. All resources are released.

     ccsCOMPL_STAT lsfSerialInit
     ccsCOMPL_STAT lsfSerialStandby
     ccsCOMPL_STAT lsfSerialOnline
     ccsCOMPL_STAT lsfSerialStop
     ccsCOMPL_STAT lsfSerialOff
     ccsCOMPL_STAT lsfSerialExit
     ccsCOMPL_STAT lsfSerialSimulat
     ccsCOMPL_STAT lsfSerialStopsim

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

54 of 81

     ccsCOMPL_STAT lsfSerialSelftest

     ccsCOMPL_STAT lsfSerialTest

                                  ( IN  lsfSERIAL_DATA *serialData,

                                    IN  const char     *serialName,

                                    OUT ccsERROR       *error )

         These methods implement the behaviour of the standard commands.

         If <serialName> is NULL, or "all" all the serials will be

         affected, otherwise only the specified one.

P RIVATE METHODS

     static ccsCOMPL_STAT lsfSerialCallHook

                                  ( IN  lsfSERIAL_DATA *serialData,

                                    IN  const char     *serialName,

                                    IN  const char     *serialFct,

                                    OUT ccsERROR       *error )

         This method invokes the user-defined hook function

         <mod>Serial<serialFct>Hook(<serialData>,<serialName>,error).

         It is invoked at Init completion only.

P RIVATE DATA MEMBERS

     The data stucture lsfSERIAL_ENTRY is a sub-class of lsfDEVICE_ENTRY.

     typedef struct

     {

       vltINT32         state;

       vltINT32         subState;

       vltLOGICAL       init;

       vltLOGICAL       simulation;

       vltINT32         timeout;

                                    Additional data members

       vltINT32         fd;            File descriptor

       vltLOGICAL       isTyCo;        True when TyCo device

     } lsfSERIAL_ENTRY;

     The data stucture lsfSERIAL_DATA is a sub-class of lsfDEVICE_DATA.

     typedef struct

     {

       void            *ctrlData;

       void            *userData;

       vltINT32         state;

       vltINT32         subState;

       vltLOGICAL       init;

       vltLOGICAL       simulation;

       vltINT32         timeout;

       vltINT32         numSerials;                    Number of serials

       vltBYTES20       *serialNames;                  Serial names

                                                      (dynamic allocated)

       char             *attrTable[lsfMAX_DEVICES+1];

       lsfSERIAL_ENTRY  *serialTable[lsfMAX_DEVICES];  Serial data

     } lsfSERIAL_DATA;

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 55 of 81

DATABASE

     The class lsfDB_SERIAL is a sub-class of lsfDB_DEVICE.
     It is partially mapped by the data structure lsfSERIAL_ENTRY.
     Each serial communication link is represented in the database by a
     point under the main serial point :control:serial, which is partially
     mapped by the data structure lsfSERIAL_DATA.
     The sub-classes lsfDB_RS232, lsfDB_RS422 and lsfDB_RS485 derive from
lsfDB_SERIAL
     whereby the protocol and handshake are overloaded.

SEE ALSO

     lsfDB_SERIAL(5)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

56 of 81

3.2.9 lsfTaskDev(3)

NAME

     lsfTaskDev - Control Task Devices

SYNOP SIS

     #include "lsfTaskDev.h"

DESCRIP TION

     This class provides the methods for the control of task devices.

     It implements the default behaviour for all the standard commands.

     Function of the state, the task devices are activated/stopped.

P UBLIC METHODS

     ccsCOMPL_STAT lsfTaskDevTrigger

                                  ( IN  lsfTASKDEV_DATA *taskDevData,

                                    IN  const char      *taskDevName,

                                    OUT ccsERROR        *error )

         This method triggers the given task asynchronously.

         If the timer is based on TIM, the activation occurs asynchronously

         within the period; otherwise, the periodic delay is restarted

         after activation.

     STATUS        lsfTaskDevVerify

                                  ( IN  lsfTASKDEV_DATA *taskDevData,

                                    IN  const char      *taskDevName,

                                    OUT ccsERROR        *error )

         This method returns the status of the given task device.

         OK if running; ERROR if not. see taskIdVerify()

         If <taskDevName> is "all" the return value is OK if all tasks

         are running otherwise ERROR;

P ROTECTED METHODS

     ccsCOMPL_STAT lsfTaskDevConstructor

                                  ( IN  const char      *swdName,

                                    IN  lsfCONTROL_DATA *controlData,

                                    IN  const char      *taskDevNames[],

                                    OUT ccsERROR        *error )

         This is the constructor of the taskDev object. It affects all the

         task devices given in the list <taskDevNames[]> (NULL terminated).

     void          lsfTaskDevDestructor

                                  ( IN  lsfCONTROL_DATA *controlData )

         This method is the object destructor. All resources are released.

     ccsCOMPL_STAT lsfTaskDevInit

     ccsCOMPL_STAT lsfTaskDevStandby

     ccsCOMPL_STAT lsfTaskDevOnline

     ccsCOMPL_STAT lsfTaskDevStop

     ccsCOMPL_STAT lsfTaskDevOff

     ccsCOMPL_STAT lsfTaskDevExit

     ccsCOMPL_STAT lsfTaskDevSimulat

     ccsCOMPL_STAT lsfTaskDevStopsim

     ccsCOMPL_STAT lsfTaskDevSelftest

     ccsCOMPL_STAT lsfTaskDevTest ( IN  lsfTASKDEV_DATA *taskDevData,

                                    IN  const char      *taskDevName,

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 57 of 81

                                    OUT ccsERROR        *error )
         These methods forward the standard commands to the task
         devices given in the list <taskDevName>.
         If <taskDevName> is NULL, or "all" all the task devices will
         be affected, otherwise only the specified one.
         It updates the state and subState of the group.

P RIVATE METHODS

     static ccsCOMPL_STAT lsfTaskDevLoop
                                  ( IN  lsfTASKDEV_DATA *taskDevData,
                                    IN  int              tskIdx,
                                    OUT ccsCOMPL_STAT   *tskStat,
                                    IN  SEM_ID          *tskSync,
                                    OUT ccsERROR        *error )
         This method is the core of the task. Therefore the structure is
         imposed. It invoked an optional prologue user function
         <mod><taskDevName>ProHook(), then enters the infinite loop
         in which it invokes the user core function <mod><taskDevName>()
         When the task is told to terminate, it invoked the optional
         epilogue user function <mod><taskDevName>EpiHook().
         All the task hook functions must comply the prototype:

           typedef ccsCOMPL_STAT lsfTASKDEV_HOOK
                                  ( IN  lsfTASKDEV_DATA *taskDevData,
                                    IN  const char      *taskDevName,
                                    OUT ccsERROR        *error)
         The function names must follow the syntax:
           <moduleName><taskDevName>["ProHook" | "" | "EpiHook"]()
         The core function <moduleName><taskDevName>() is mandatory.

     static ccsCOMPL_STAT lsfTaskDevActivate
                                  ( IN  lsfTASKDEV_DATA *taskDevData,
                                    IN  int              tskIdx,
                                    OUT ccsERROR        *error )
         This method activates the task indexed <tskIdx>.

     static ccsCOMPL_STAT lsfTaskDevSchedule
                                  ( IN  lsfTASKDEV_DATA *taskDevData,
                                    IN  const char      *taskDevName,
                                    IN  vltINT32         state,
                                    OUT ccsERROR        *error )
         This method schedules the tasks depending on their start state.
         If the <state> is higher or equal the start state, the task is
         activated, otherwise it is terminated.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

58 of 81

P RIVATE DATA MEMBERS

     The data stucture lsfTASKDEV_ENTRY is a sub-class of lsfDEVICE_ENTRY.

     typedef struct

     {

       vltINT32         state;

       vltINT32         subState;

       vltLOGICAL       init;

       vltLOGICAL       simulation;

       vltINT32         timeout;

                                    Additional data members

       vltINT32      startState;       Miniumum state for schedule

       vltLOGICAL    ignoreStop;       True when stop is ignored

       vltLOGICAL    first;            True when starting

       vltINT32      tcb,tid;          Task TCB for lccTaskLib

       void         *fctHook[3];       Addresses of function hooks

     } lsfTASKDEV_ENTRY;

     The data stucture lsfTASKDEV_DATA is a sub-class of lsfDEVICE_DATA.

     typedef struct

     {

       void             *ctrlData;

       void             *userData;

       vltINT32          state;

       vltINT32          subState;

       vltLOGICAL        init;

       vltLOGICAL        simulation;

       vltINT32          timeout;

       vltINT32          numTaskDevs;         Number of tasks

       vltBYTES20       *taskDevNames;        Names of the tasks

                                                      (dynamic allocated)

       char             *attrTable[lsfMAX_DEVICES+1];

       lsfTASKDEV_ENTRY *taskDevTable[lsfMAX_DEVICES];   TaskDev data

     } lsfTASKDEV_DATA;

DATABASE

     The class lsfDB_TASKDEV is a sub-class of lsfDB_DEVICE.

     It is partially mapped by the data structure lsfTASKDEV_ENTRY.

     Each task is represented in the database by a point under the

     main point :control:taskDev, which is partially mapped by the data

     structure lsfTASKDEV_DATA.

SEE ALSO

     lsfDB_DEVICE(5)

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 59 of 81

3.2.10 lsfSoftDev(3)

NAME

     lsfSoftDev - Control underlying Software Devices

SYNOP SIS

     #include "lsfSoftDev.h"

DESCRIP TION

     This class provides the methods for the control of software devices.
     It implements the default behaviour for all the standard commands.
     The standard commands are forwarded to the underlying software devices.

P UBLIC METHODS

     ccsCOMPL_STAT lsfForwardCommand
                                  ( IN  lsfSOFTDEV_DATA *softDevData,
                                    IN  const char      *softDevName,
                                    IN  const char      *command,
                                    IN  const char      *param,
                                    OUT char            *reply,
                                    OUT ccsERROR        *error )
         This method forward a command to the software devices specified
         by <softDevName>. If <softDevName> is NULL, or "all" all the
         software devices will be affected, otherwise only the specified one.
         The method returns the completion status of the command, thus waits
         for all specified software devices to reply.

P ROTECTED METHODS

     ccsCOMPL_STAT lsfSoftDevConstructor
                                  ( IN  const char      *swdName,
                                    IN  lsfCONTROL_DATA *controlData,
                                    IN  const char      *softDevNames[],
                                    OUT ccsERROR        *error )
         This is the constructor of the softDev object. It affects all the
         software devices given in the list <softDevNames[]> (NULL terminated).
     void          lsfSoftDevDestructor
                                  ( IN  lsfCONTROL_DATA *controlData )
         This method is the object destructor. All resources are released.

     ccsCOMPL_STAT lsfSoftDevInit
     ccsCOMPL_STAT lsfSoftDevStandby
     ccsCOMPL_STAT lsfSoftDevOnline
     ccsCOMPL_STAT lsfSoftDevStop
     ccsCOMPL_STAT lsfSoftDevOff
     ccsCOMPL_STAT lsfSoftDevExit
     ccsCOMPL_STAT lsfSoftDevSimulat
     ccsCOMPL_STAT lsfSoftDevStopsim
     ccsCOMPL_STAT lsfSoftDevSelftest
     ccsCOMPL_STAT lsfSoftDevTest ( IN  lsfSOFTDEV_DATA *softDevData,
                                    IN  const char      *softDevName,
                                    OUT ccsERROR        *error )
         These methods forward the standard commands to the software
         devices given ib the list <softDevName>.
         If <softDevName> is NULL, or "all" all the software devices will
         be affected, otherwise only the specified one.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

60 of 81

         It updates the state and subState of the group.

P RIVATE METHODS

     static ccsCOMPL_STAT lsfSendCommand

                                  ( IN  const char *srvName,

                                    IN  const char *command,

                                    IN  const char *param,

                                    OUT ccsERROR   *error )

         This method sends the command <command> with the

         parameters <param> to the server process <srvName> of the

         software device.

     static ccsCOMPL_STAT lsfWaitReply

                                  ( IN  const char *srvName,

                                    IN  const char *command,

                                    IN  char       *reply,

                                    IN  int         timeout,

                                    OUT ccsERROR   *error )

         This method waits for the last or error reply to the command

         <command> from the server process <srvName> of the software device.

         The reply is stored in <reply>.

P RIVATE DATA MEMBERS

     The data stucture lsfSOFTDEV_ENTRY is a sub-class of lsfDEVICE_ENTRY.

     typedef struct

     {

       vltINT32         state;

       vltINT32         subState;

       vltLOGICAL       init;

       vltLOGICAL       simulation;

       vltINT32         timeout;

                                    Additional data members

       vltBYTES20  serverName;          Name of the server process

     } lsfSOFTDEV_ENTRY;

     The data stucture lsfSOFTDEV_DATA is a sub-class of lsfDEVICE_DATA.

     typedef struct

     {

       void             *ctrlData;

       void             *userData;

       vltINT32          state;

       vltINT32          subState;

       vltLOGICAL        init;

       vltLOGICAL        simulation;

       vltINT32          timeout;

       vltINT32          numSoftDevs;         Number of software devices

       vltBYTES20       *softDevNames;        Names of the software devices

                                                      (dynamic allocated)

       char             *attrTable[lsfMAX_DEVICES+1];

       lsfSOFTDEV_ENTRY *softDevTable[lsfMAX_DEVICES];   SoftDev data

     } lsfSOFTDEV_DATA;

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

63 of 81

#ifdef lsfNUM_NETWORK

#if lsfNUM_NETWORK > 0

    ATTRIBUTE  "lsfDB_DEVICE"  lsfDEVTYPE_NETWORK_STR

#endif

#endif

#ifdef lsfNUM_SOFTDEV

#if lsfNUM_SOFTDEV > 0

    ATTRIBUTE  "lsfDB_DEVICE"  lsfDEVTYPE_SOFTDEV_STR

#endif

#endif

#ifdef lsfNUM_TASKDEV

#if lsfNUM_TASKDEV > 0

    ATTRIBUTE  "lsfDB_DEVICE"  lsfDEVTYPE_TASKDEV_STR

#endif

#endif

END

#endif

#endif

CLASS "lsfDB_SERVER" "pfxDB_SERVER"

BEGIN

#ifdef lsfNUM_DEVICES

    ATTRIBUTE int32     numDevices lsfNUM_DEVICES

#if lsfNUM_DEVICES > 0

    ATTRIBUTE "pfxDB_CONTROL" control

    BEGIN

        ATTRIBUTE Table deviceTable (lsfNUM_DEVICES)

    END

#endif

#else

    ATTRIBUTE int32     numDevices 0

#endif

    ATTRIBUTE "pfxDB_DATA" data

END

POINT "pfxDB_SERVER" pfxDB_ROOT

BEGIN

    ALIAS pfxMODULE_NAME

//

// Instanciate all devices

//

#ifdef lsfNUM_DEVICES

#if lsfNUM_DEVICES > 0

//  ATTRIBUTE "<lsfDB_CLASS>"   control:<devType1>:<devName1>

//  ATTRIBUTE "<pfxDB_CLASS>"   control:<devType2>:<devName2>

#endif

#endif

END

// END OF FILE

// ============================================================

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 64 of 81

3.3.2 lsfDB_SERVER(5)

NAME

     lsfDB_SERVER - Base class for software device application

SYNOP SIS

     #include "lsfDB_SERVER.class"
     POINT lsfDB_SERVER ":<myPath>:<myMod>"
     BEGIN
       ALIAS "myMod"
     END

P ARENT CLASS

     lsfDB_DEVICE <-- lsfDB_SOFTDEV <-- lsfDB_SERVER

DESCRIP TION

     The class lsfDB_SERVER is the generic definition of the top point of
     a software device. It holds the minimum information required
     by "lsf" for the software device management.

ATTRIBUTES

     In addition to those defined in the parent class lsfDB_SOFTDEV:
       monPeriod   : period in ms of the associated monitor task
       numDevices  : number of controlled devices

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

65 of 81

3.3.3 lsfDB_CONTROL(5)

NAME

     lsfDB_CONTROL - Base class for application control point

SYNOP SIS

     #include "lsfDB_CONTROL.class"

     ATTRIBUTE lsfDB_CONTROL control

P ARENT CLASS

     BASE_CLASS <-- lsfDB_CONTROL

DESCRIP TION

     The class lsfDB_CONTROL is the generic definition of the

     control point.

     It contains the attribute <deviceTable> holding the information

     relevant to the control of the devices.

     The application control point is instanciated from a sub-class

     of this generic class. In particular it overloads the number of

     devices and adds a sub-point per device type.

ATTRIBUTES

   - TABLE deviceTable(1)

       deviceName : name of the device

       deviceType : type of the device

       startPhase : sequence order when increasing the device state

       stopPhase  : sequence order when decreasing the device state

       simulation : true if device shall be controlled in simulation

       ignored    : true is device shall be ignored

CAUTIONS

       The two fields <startPhase> and <stopPhase> are ignored.

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 66 of 81

3.3.4 lsfDB_DATA(5)

NAME

   lsfDB_DATA - Base class for application data

SYNOP SIS

     #include "lsfDB_DATA.class"

     ATTRIBUTE lsfDB_DATA data

P ARENT CLASS

     BASE_CLASS <-- lsfDB_DATA

DESCRIP TION

     This class is the generic definition of the data point.
     It is provided to hold the application specific data used e.g.
     for monitoring purpose.
     The application data point is instanciated from a sub-class
     of this generic class. Its definition is application dependent.

ATTRIBUTES

     None

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

67 of 81

3.3.5 lsfDB_DEVICE(5)

NAME

   lsfDB_DEVICE - Base class for devices

SYNOP SIS

     #include "lsfDB_DEVICE.class"

     ATTRIBUTE lsfDB_DEVICE  <aGenericDevice>

P ARENT CLASS

     BASE_CLASS <-- lsfDB_DEVICE

DESCRIP TION

     The class lsfDB_DEVICE is the generic definition of a device.

     It holds the minimum information required by "lsf" for the

     device management. For each type of device a specialized

     sub-class is provided that adds specific attributes.

ATTRIBUTES

     lsfDB_DEVICE

       state       : state of the device (= LCC states)

       substate    : sub-state of the device

       initialized : true if device is initialized

       simulation  : true if device shall be controlled in simulation

       timeout     : timeout in seconds for command execution

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 68 of 81

3.3.6 lsfDB_SIGNAL(5)

NAME

   lsfDB_SIGNAL - Base classes for analogue and digital signals

SYNOP SIS

     #include "lsfDB_SIGNAL.class"

     ATTRIBUTE lsfDB_ANALOG  analog
     ATTRIBUTE lsfDB_DIGITAL digital

P ARENT CLASS

                                      |-- lsfDB_ANALOG
     lsfDB_DEVICE <-- lsfDB_SIGNAL <--+
                                      |-- lsfDB_DIGITAL

DESCRIP TION

     The class lsfDB_SIGNAL is the generic definition of a signal
     (analogue or digital) device. It contains the attribute holding
     the information relevant to the control of these devices.

ATTRIBUTES

     The following attributes are mapping for Analog and Digital
     signals the configuration parameters expexted by the LCC
     functions ioConfigAnalog(3), resp. ioConfigDigital(3).

     lsfDB_SIGNAL
       In addition to those defined in the parent class lsfDB_DEVICE:
         deviceName : name of the device "/acroN" for Digital signals
                                         "/aioN"  for Analogue signals
         direction  : signal direction (Input/Output)

     lsfDB_ANALOG
         deviceName : overloaded to "/aio"
       In addition to those defined in the parent class lsfDB_SIGNAL:
         channel    : channel number
         gain       : amplifier gain
         conversionFactor: floating point value
         lowerRange : signal range
         higherRange:
         simValue   : simulation value
         signalA    : associated database point (lccANALOG_SIGNAL)

     lsfDB_DIGITAL
         deviceName : overloaded to "/acro"
       In addition to those defined in the parent class lsfDB_SIGNAL:
         level      : active Low/High
         startBit   : lower bit [0-63]
         numBits    : number of bits mapping the signal
         simValue   : simulation value
         signalD    : associated database point (lccDIGITAL_SIGNAL)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

69 of 81

SEE ALSO

     LCC User Manual for Signal Handling

     ioConfigAnalog(3), ioConfigDigital(3)

     Digital I/O Board User Manual, and acro driver User Manual

     Analog  I/O Board User Manual, and aio  driver User Manual

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 70 of 81

3.3.7 lsfDB_MOTOR(5) NAME

   lsfDB_MOTOR - Base class for motor

SYNOP SIS

     #include "lsfDB_MOTOR.class"
     ATTRIBUTE lsfDB_MOTOR <aMotorDevice>

P ARENT CLASS

     lsfDB_DEVICE <-- lsfDB_MOTOR

DESCRIP TION

     The class lsfDB_MOTOR is the specialized class for motors of
     any kind.
     At instanciation, the class of the attribute <motor> shall be
     overloaded with the sub-class corresponding to the motor.

ATTRIBUTES

     In addition to those defined in the parent class lsfDB_DEVICE:
       motor : motor branch (from motMOTOR)

SEE ALSO

     motor.db(5), motMOTORS(5)

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

71 of 81

3.3.8 lsfDB_SERIAL(5)

NAME

   lsfDB_SERIAL - Base classes for serial communication links

SYNOP SIS

     ATTRIBUTE lsfDB_SERIAL com

     ATTRIBUTE lsfDB_RS232  com1

     ATTRIBUTE lsfDB_RS422  com2

     ATTRIBUTE lsfDB_RS485  com3

P ARENT CLASS

                                      |-- lsfDB_RS232

     lsfDB_DEVICE <-- lsfDB_SERIAL <--+-- lsfDB_RS422

                                      |-- lsfDB_RS485

DESCRIP TION

     The class lsfDB_SERIAL is the generic definition of a serial

     communication device. It contains the attribute holding the

     information relevant to the control of these devices.

     The 3 sub-classes lsfDB_RS232, lsfDB_RS422 and lsfDB_RS485 are

     specialized classes for the control of RS232, RS422 and RS485 resp.

     communication links based on these protocols.

ATTRIBUTES

     lsfDB_SERIAL

       In addition to those defined in the parent class lsfDB_DEVICE:

       deviceName  : name of the device "/iser0-9" or "/tyCo/1-3"

       protocol    : number of the RS protocol [232, 422 or 485]

       for the following attributes, see iserDrv(3) and VxWorks

       manuals for tyCo devices

       baudRate    :

       dataBits    :

       stopBits    :

       parity      :

       handShake   :

       rxMode      :

       bufferLength:

    lsfDB_RS232, lsfDB_RS422 and lsfDB_RS485: these sub-classes overload

      the attributes ’protocol’ and ’handShake’.

SEE ALSO

    iserDrv(3), VxWorks tyLib(1), ttyLib(1) and related

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 72 of 81

3.3.9 lsfDB_TASKDEV(5)

NAME

   lsfDB_TASKDEV - Base classes for task devices

SYNOP SIS

     #include "lsfDB_TASKDEV.class"

     ATTRIBUTE lsfDB_TASKDEV <aTaskDevice>

P ARENT CLASS

     lsfDB_DEVICE <-- lsfDB_TASKDEV

DESCRIP TION

     The class lsfDB_TASKDEV is the specialized class for tasks
     devices to be controlled by the application.

ATTRIBUTES

     lsfDB_TASKDEV
       In addition to those defined in the parent class lsfDB_DEVICE:
       startState  : minimum state for task activation
       timerNum    : timer number for period
                        -1 : use system call taskDelay()
                     1 - 4 : use TIM timer
       period      : task period in milli-seconds
       priority    : task priority
       stackSize   : task stack size in kilo-bytes [kB]

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

73 of 81

3.3.10 lsfDB_SOFTDEV(5)

NAME

   lsfDB_SOFTDEV - Base classes for software devices

SYNOP SIS

     #include "lsfDB_SOFTDEV.class"

     ATTRIBUTE lsfDB_SOFTDEV <aSoftwareDevice>

P ARENT CLASS

     lsfDB_DEVICE <-- lsfDB_SOFTDEV

DESCRIP TION

     The class lsfDB_SOFTDEV is the specialized class for Software

     devices to be controlled by the application.

ATTRIBUTES

     lsfDB_SOFTDEV

       In addition to those defined in the parent class lsfDB_DEVICE:

       serverName  : name of the software device server

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 74 of 81

3.4 Include Files

3.4.1 lsfDefines.h

#ifndef LSF_DEFINES_H
#define LSF_DEFINES_H
/*******************************************************************************
* E.S.O. - VLT project
*
* "@(#) $Id: lsfDefines.h,v 1.27 2000/10/24 08:32:16 vltsccm Exp $"
*
* who       when        what
* --------  ----------  ----------------------------------------------
* pduhoux   2000-04-10  created
*/

/************************************************************************
 *
 *----------------------------------------------------------------------
 */

/*
 * Constants
 */
#define _eccs_tostr(a) #a
#define _eccs_tostr_pass2(a) _eccs_tostr(a)

#define __FILE_LINE__  __FILE__ ":" _eccs_tostr_pass2(__LINE__)

#define lsfMODULE_ID    "lsf" /* module name */
#define lsfMODULE_NAME   lsfMODULE_ID
#define lsfMODULE_TITLE  "LCU Server Framework"
#define lsfLOG_ID  100

#define lsfMAX_DEVICES          32

/*
 * Database
 */
#define lsfDB_CONTROL_POINT    ":control"
#define lsfDB_DATA_POINT       ":data"

#define lsfDB_SIGNAL_POINT     ":signal"
#define lsfDB_MOTOR_POINT      ":motor"
#define lsfDB_SERIAL_POINT     ":serial"
#define lsfDB_ENCODER_POINT    ":encoder"
#define lsfDB_NETWORK_POINT    ":network"
#define lsfDB_SOFTDEV_POINT    ":softdev"
#define lsfDB_TASKDEV_POINT    ":taskdev"

#define lsfALL_DEVICES         "all"

#define lsfDEVTYPE_SIGNAL_STR     "signal"
#define   lsfDEVTYPE_ANALOG_STR   "analog"
#define   lsfDEVTYPE_DIGITAL_STR  "digital"
#define lsfDEVTYPE_MOTOR_STR      "motor"
#define lsfDEVTYPE_SERIAL_STR     "serial"
#define   lsfDEVTYPE_TYCO_STR     "tyCo"
#define   lsfDEVTYPE_RS232_STR    "rs232"
#define   lsfDEVTYPE_RS422_STR    "rs422"

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

75 of 81

#define   lsfDEVTYPE_RS485_STR    "rs485"

#define lsfDEVTYPE_ENCODER_STR    "encoder"

#define   lsfDEVTYPE_IK320_STR    "ik320"

#define lsfDEVTYPE_NETWORK_STR    "network"

#define   lsfDEVTYPE_ETHERNET_STR "ethernet"

#define   lsfDEVTYPE_NET01_STR    "net01"

#define   lsfDEVTYPE_ATM_STR      "atm"

#define lsfDEVTYPE_SOFTDEV_STR    "softdev"

#define lsfDEVTYPE_TASKDEV_STR    "taskdev"

#define lsfDEVICE_NUM_TYPES 7

#define lsfDEVICE_SIGNAL    1

#define lsfDEVICE_MOTOR     2

#define lsfDEVICE_SERIAL    3

#define lsfDEVICE_ENCODER   4

#define lsfDEVICE_NETWORK   5

#define lsfDEVICE_SOFTDEV   6

#define lsfDEVICE_TASKDEV   7

/* lsfDEVTYPE_<device> = (0x100 << (lsfDEVICE_<type>-1)) + <kind> */

#define lsfDEVTYPE_MASK       0xFF00

#define lsfDEVTYPE_UNKNOWN    0

#define lsfDEVTYPE_SIGNAL     0x0100

#define   lsfDEVTYPE_ANALOG   0x0101      /* = lsfDEVTYPE_SIGNAL | ioANALOG */

#define   lsfDEVTYPE_DIGITAL  0x0102      /* = lsfDEVTYPE_SIGNAL | ioDIGITAL */

#define lsfDEVTYPE_MOTOR      0x0200

#define lsfDEVTYPE_SERIAL     0x0400

#define   lsfDEVTYPE_RS232    0x0401

#define   lsfDEVTYPE_RS422    0x0402

#define   lsfDEVTYPE_RS485    0x0404

#define lsfDEVTYPE_ENCODER    0x0800

#define   lsfDEVTYPE_IK320    0x0801

#define lsfDEVTYPE_NETWORK    0x1000

#define   lsfDEVTYPE_ETHERNET 0x1001

#define   lsfDEVTYPE_NET01    0x1002

#define   lsfDEVTYPE_ATM      0x1004

#define lsfDEVTYPE_SOFTDEV    0x2000

#define lsfDEVTYPE_TASKDEV    0x4000

#define lsfSTATE_OFF     1

#define lsfSTATE_LOADED  2

#define lsfSTATE_STANDBY 3

#define lsfSTATE_ONLINE  4

#define lsfUNCHANGED -99

#define lsfSUBSTATE_IDLE         0

#define lsfSUBSTATE_ERROR        1

#define lsfSUBSTATE_TIMEOUT      2

#define lsfSUBSTATE_INITIALIZING 3

#define lsfSUBSTATE_ACTIVE       4

#define lsfSUBSTATE_MONITORING   5

#define lsfSUBSTATE_MOVING       6

#define lsfSUBSTATE_WAITING      7

#define lsfATTR_NAMES \

    "state","substate","simulation","initialized","timeout"

#define lsfDB_STATE          0

#define lsfDB_SUBSTATE       1

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

78 of 81 ordinating Software Device to the sub-ordinated ones, any standard command sent to

LCC (process lccServer) would be forwarded to all the registered Software Devices found in this list, but as well from the co-ordinating Software Devices to the subordinated ones resulting in non predictable effects.

• Configure the LCU bootScript and reboot the LCU:

      > vccConfigLcu lcuEnv &

      >

In the LCU Configuration panel:

1. Update the user module list that shall contain:

lsf and app in this precedence order.

For applications that do use motors, the module mcm must be added.

2. Add the required driver devices,

3. Add the process appServer.

4. Click on the button Write Files to save the configuration

5. Click on the button Reboot LCU to boot the LCU

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 79 of 81

4.1.3 Scan Links

After both environments have been successfully started, the scan links can be configured. Edit the file

app/ws/config/app.scan to add all the links required by the application.

Example:

> cd app/ws/config
> vi app.scan
 ...
> cd ../src
> make install
 ...
 . . . installation done
>
> scanLinks -f $INTROOT/config/app.scan -l wsEnv -e lcuEnv -c -E -r <path>
>

where <path> is the absolute path of the database root point of the application on the WS.

ESO_{LCU Common Software}

LCU Server Framework

User Manual Doc.

Issue

Date

Page VLT-MAN-ESO-17210-2252 1.0 2000-10-25

80 of 81

The WS database will now be kept aligned with the LCU database by means of the scan system. In particular, the module state and sub-state are updated on change (mode SRBX).

4.1.4 Verification

On the Workstation, invoke the panel appgui.

The fields State, Substate and Mode shall not be shaded (indication for bad data quality, hence scan troubles). They shall indicate LOADED (in Orange), IDLE (in Green) and NORMAL (in Green) resp.

Send the command VERSION.

The Software Device is ready for use, however it might be necessary to tune the configuration of the devices (e.g. motors or signals).

4.1.5 Database configuration

This last section is dedicated to the handling of the database configuration file of the application

(app/ws/config/app.dbcfg).

As mentioned above, this file is generated by the utility lsfConfig(1). It contains then the minimum necessary configuration attributes for the software device to startup. After the tuning of the hardware has been completed, i.e. all devices are properly configured and initialize and perform as required, the database shall be saved into the file app/ws/config/app.dbcfg by means of the utility lsfBackup(1).

Example:

> cd app/ws/config

> lsfBackup -e lcuEnv -m app

Generating input file ’./app.inp’ ... done

Performing database backup into ’app.dbcfg’ ... done

> cd ../src

> make install

 ...

 . . . installation done

>

Last modified: Thu Sep 28 10:32:15 METDST 2000

ESO^{LCU Common Software}

LCU Server Framework User Manual

Doc. Issue Date Page

VLT-MAN-ESO-17210-2252 1.0 2000-10-25 81 of 81

___oOo___