NEW TECHNOLOGY TELESCOPE EMMI/S USI2 MORNING CALIBRATION FORM

LSO-FOR-ESO-40610-0001/1.1, 20/11/1998

Prepared: J.-F. Gonzalez, Approved: Hainaut, Released: O.Hainaut

The observers are reminded that they are entitled to UP TO 2 HOURS of calibrations taken in the morning by the NTT staff, including standard Calibration Plan OBs, Please start the BIASES and DARKS before leaving the telescope in the morning.

Name: Prog. ID: Date:

Standard Calibration Plan Obser vation Blocks

Obser vation Readout Speed

Detector Optical Elements Fixed Parameters

9 Biases EMMI^{Slow}_{Normal}

Fast

Blue Red No windowing Binning 1 1

9 Biases SuSI2^{Normal SuSI2 No windowing}_{Binning 2x2}

1 Dark EMMI^{Slow}_{Normal}

Fast

Blue Red No windowing Binning 1 1 30 min

1 Dark SuSI2^{Normal SuSI2 No windowing}_{Binning 2 2}

30 min

3 Imaging Dome Flats

EMMI

Slow Normal Fast

Blue U#602 B#603 B#604

No windowing Binning 1 1 20 000 ADU Red Bb#605

V#606 R#608 I#610 Z#611 g#772 r#773 i#774 z#775

3 Imaging Dome Flats

SuSI2

Normal SuSI2 U#810 U#823 B#811 V#812

R#813 I#814 Z#815 r#822

No windowing Binning 2 2 20 000 ADU

3 LD Spectroscop^y

Dome Flats EMMI

Slow Normal Fast

Red Slit 1”

Slit 5”

Gr#1 Gr#2

Gr#3 Gr#4 Gr#5 Gr#6 Gr#7

No windowing Binning 1 1 20 000 ADU

1 LD Spectroscop^y

Wavelength Calibration EMMI

Fast Red Gr#1 Gr#2 Gr#3 Gr#4

Gr#5 Gr#6 Gr#7

No windowing Binning 1 1 Slit 1” He+Ar Std exp. time

Please write down the names of your calibration OBs, ordered by priority.

User-Defined Obser vation Blocks

P2PP ID: Passwd:

OB Name Lighting Conditions

(Internal Lamps/Dome Lamps/Dome Flaps)

Estimated Duration

Comments: